; Copyright (c) Anyka Cayman Corporation.  All rights reserved.
;               
; usbanyka.inf - Anyka USB Web Camera install file
;

[Version]
LayoutFile=layout.inf
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%OrganizationName%
CatalogFile=usbanyka.cat ; This file is required and is supplied when the package is certified
DriverVer=09/05/2006,1.00.02.00

[SourceDisksNames]
1000 = %cdname%,,,

[ControlFlags]
; All PnP devices should be excluded from manual AddDevice Applet list
ExcludeFromSelect=*

[Manufacturer]
%AnykaMfg%=Anyka

[DestinationDirs]
Anyka.USBDCam.Files=10,system32\drivers

[Anyka]
%USB\VID_04D6&PID_065F.DeviceDesc%=Anyka.USBDCam,USB\VID_04D6&PID_065F

[Anyka.USBDCam.NT]
Include=    ks.inf, kscaptur.inf, dshowext.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,DSHOWEXT.Registration
AddReg=     Anyka.USBDCam.AddReg
CopyFiles=Anyka.USBDCam.Files
;WIA
SubClass=StillImage
DeviceType=3
DeviceSubType=0x1
Capabilities=0x00000031
DeviceData=Anyka.USBDCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"

[Anyka.USBDCam.AddReg]
;HKR,,OkToHibernate,3,01
;HKR,,DontSuspendIfStreamsAreRunning,3,01
;HKR,,PageOutWhenUnopened,3,01
;HKR,Settings,Brightness,0x00010001,0x3c
;HKR,Settings,Contrast,0x00010001,0x30
;HKR,Settings,Saturation,0x00010001,0x54
;HKR,Settings,Sharpness,0x00010001,0x54
;HKR,Settings,WhiteBalance,0x00010001,0x114
; WIA
HKR,,HardwareConfig,1,1
HKR,,USDClass,,"{0527d1d0-88c2-11d2-82c7-00c04f8ec183}"

[Anyka.USBDCam.DeviceData]
Server=local
UI Class ID={5d8ef5a3-ac13-11d2-a093-00c04f72dc3c}

[Anyka.USBDCam.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,Anyka.USBDCam.Interface
AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,Anyka.USBDCam.Interface

[Anyka.USBDCam.Interface]
AddReg=Anyka.USBDCam.Intf.AddReg
         
[Anyka.USBDCam.Intf.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,FriendlyName,,%USB\VID_04D6&PID_065F.DeviceDesc%
HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,21,E8,C2,3D, 13,47, d2,11, 0xba, 0x41, 0x0, 0xa0, 0xc9, 0xd, 0x2b, 0x5
HKR,PinFactory\1\Interfaces\{5BB95400-52BB-11d2-BA41-00A0C90D2B05},,,

[Anyka.USBDCam.NT.Services]
AddService = usbanyka,0x00000002,Anyka.USBDCam.ServiceInstall

[Anyka.USBDCam.ServiceInstall]
DisplayName   = %USB\VID_04D6&PID_065F.DeviceDesc%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\UsbAnyka.sys

[Anyka.USBDCam.Files]
usbanyka.sys
usbcamd.sys
stream.sys

[Strings]

;----------------
; Non-Localizable
;----------------

ProxyVCap.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO="{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
SERVICE_KERNEL_DRIVER=1
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1

;----------------
; Localizable
;----------------

OrganizationName="Anyka (Guangzhou) Software Technology Co., Ltd."

AnykaMfg="Anyka"
USB\VID_04D6&PID_065F.DeviceDesc="Anyka USB Web Camera"

cdname="Disk 1"


