CECInfo
(
	Name ( ".Dll EETI" )
	CECVersion ( 4.20 )
	Description ( "EETI RS232 Touch Screen Driver" )
	GUID ( {B4513333-5027-4FF9-9A9F-0B3BB2DA5CD4} )
	Vendor ( "EETI Inc." )
)
ComponentType
(
	Name ( "Touch" )
	GUID ( {94D33DF5-5A3D-46FA-A704-1C1E6793E0CB} )
	Description ( "eeti RS232 Touch Driver" )
	Group ( "\Device Drivers\Touch" )
	Vendor ( "EETI" )
	MaxResolvedImpsAllowed( 1 )
	Implementations
	(
		Implementation
		(
			Name ( "eeti RS232" )
			GUID ( {6AD2088F-BE44-463D-A39C-B82A8852CB52} )
			Description ( "eeti RS232 Touch Driver" )
			Version ( "2.0.14.6019" )
			Locale ( 0409 )
			Vendor ( "eeti" )
			Date ( "2007/10/9" )
			Variable( "MODULE_NAME", "touchkit.dll" )
			SizeIsCPUDependent( 1 )
			BuildMethods
			(
				BuildMethod
				(
					GUID ( {0C08EA9B-67E1-45EF-A1A7-2FFF1CD0CFE3} )
					Step ( CESYSGEN )
					CPU ( "ARMV4" )
					CPU ( "ARMV4I" )
					CPU ( "emulator" )
					CPU ( "MIPSII" )
					CPU ( "MIPSII_FP" )
					CPU ( "MIPSIV" )
					CPU ( "MIPSIV_FP" )
					CPU ( "SH3" )
					CPU ( "SH4" )
					CPU ( "x86" )
					Action ( '#SRCCODE( USER_PROJECT, "C:\EETICEDB\wince500\eeti232.pbpxml" )' )
				)
			)
		)
	)
)
