;
; VAG-COM label file
;
; Audi A8 (4E)
;
; component: J285 - Instrument Cluster (#17)
;
; p/n: 
;
; includes coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4E-17.LBL
; 4E0-920-9xx.LBL
;
; by Sebastian Stange
; sebastian@ross-tech.com
;
; last modification: 10/02/2004
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,J285 - Instrument Cluster;
C1,??xxx - Additional Settings
C2,+01 - 2nd fuel tank map/all wheel drive coding
C3,+04 - Vehicle with clutch (not automatic)
C4,+08 - 2nd tire size pair (with differentiation between Summer and Winter tires)
C5,+16 - Tire Monitoring System (MY 2005 >)
C6,0x?xx - Country coding
C7,0 - Germany / 1 - Rest of the world (left hand) / 2 - USA / 3 - Canada
C8,4 - Great Britain / 5 - Japan (left hand) / 6 - Arab states
C9,7 - Australia / 8 - Rest of the world (right hand) / 9 - Japan (right hand)
C10,0xx?x - Seat belt warning (3-6 only MY 2005 and above)
C11,0 - No Seat belt warning  / 1 - Seat belt warning (EU-NCAP)
C13,2 - Seat belt warning (USA/Canada old) / 3 - Seat belt warning (USA/Canada NAR new)
C14,4 - Seat belt warning (EU-NCAP incl. passenger) / 5 - Seat belt warning (USA/Canada old incl. passenger)
C15,6 - Seat belt warning (USA/Canada NAR new incl. passenger)
C16,0xxx? - Illumination options (0-4 without parking light LED | 5-9 with parking light LED)
C17,0/5 - Needle and scales OFF (term.15 On/term.58 Off) | 1/6 - Needle ON scales OFF (term.15 On/term.58 Off)
C18,2/7 - Needle OFF scales ON (term.15 On/term.58 Off) | 3/8 - Needle and scales ON (term.15 On/term.58 Off)
C19,4/9 - Needle and scales ON (term.15 Off/term.58 Off)
;
