; VAG-COM Measuring Block Labels 
; VW Golf 1.4 (1998-2001)
; Code: AHW,AKQ
; ECU:  036 906 014AN (MARELLI 4CV)
; Also: MARELLI 4AV
;
; File created by:
;   Charles D.H. Williams <c.d.h.williams@ex.ac.uk>
;
;0,0,Measured Value Block
;0,1,Air intake temp,156-44 = 15-70 C
;0,2,Battery voltage,120-160 = 12.0-14.5V
;0,3,Engine temp,37-18 = 80-110 C
;0,4,Air intake pressure,32-71 = 240-420mbar
;0,5,Lambda probe voltage,0-184 = 0.00-0.90V
;0,6,Lambda control
;0,7,Not used,0
;0,8,Throttle pot.,200-240 = 4.0-4.5V
;0,9,Injection period,5-14 = 3.00-7.00ms
;0,10,Engine speed,21-25 = 700-800rpm
;
1,0,Engine - Basic State
1,1,Engine speed,700-800
1,2,Coolant temp.,85-110
1,3,Lambda probe,0.000-0.900
1,4,Conditions,00000000
;              1        -A fault is stored in memory
;               1       -Gear box intervention during gear shift
;                1      -Air conditioner compressor on
;                 1     -Idling switch (F60) open
;                  1    -Fault in lambda control
;                   1   -Throttle valve open
;                    1  -Engine speed above 1800rpm
;                     1 -Coolant temp below 80C
;
2,0,Engine - Basic State
2,1,Engine speed,700-800
2,2,Injection period,2.56-5.12
2,3,ECU supply,11.5-14.5
2,4,Air intake temp,15-70
;
3,0,Engine - Basic State
3,1,Engine speed,700-800
3,2,Engine load,12-40
3,3,Throttle angle,1-7
3,4,TV positioner,duty cycle
;
4,0,Engine - Operating Mode
4,1,Engine speed,700-800
4,2,Engine load,12-40
4,3,Vehicle speed,0
4,4,OR-ID-PT-FT,0100XXXX
;   Overrun/Idling/Part throttle/Full throttle
;
5,0,Throttle Valve Control - Operating Condition
5,1,Engine speed,700-800
5,2,Filter duty,6.0-19.0
5,3,Fuel usage,0.50-1.10
5,4,TV cal.,XX000000
;             1      -Battery Voltage too low
;              1     -Speed signal recognised
;               1    -F60 open before basic setting
;                1   -Implausible signal between G88&G69
;                 1  -Voltage Between G88&G69 out of tol.
;                  1 -F60 open during basic setting
;
6,0,Engine - Basic State
6,1,Mixture correction
6,2,Unused
6,3,Unused
6,4,Throttle,cal. param.
;
98,0,Adapting Throttle Control Basic Setting
98,1,Throttle G69,0.500-5.000
98,2,Throttle G88,0.500-5.000
98,3,Engine mode
98,4,Adaptation mode,Idle/OK/ERROR
;
