;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; component: Control Module for Telematics - J526 - (#75) (analog OnStar three button system)
;
;       p/n: 3D0 035 617 Telematik NAR1 0101 Coding: 0061860 (Phaeton - North America)
;
; includes some measured value blocks and coding - data is incomplete.
;
; by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modification: 27/March/2005
;
; ready for VAG-COM 402.3 and above
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
C00,Phaeton (3D) - Telematics System (J526) Coding
C01,61850 - Phaeton with 8 Channel Soundsystem
C02,61860 - Phaeton with 12 Channel Soundsystem
C03,61851 - Phaeton with 8 Channel Soundsystem - Information sent to Indicator Unit in Instrument Panel Insert
C04,61861 - Phaeton with 12 Channel Soundsystem - Information sent to Indicator Unit in Instrument Panel Insert
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
001,0,Telephone Signal Strength Available
;
002,0,GPS Satellite Status for OnStar System
;
003,0,Status of Automatically Generated Breakdown Signal (e.g. airbag deployment)
;
004,0,Status of Red (emergency) Button
;
005,0,Vehicle Electrical System Status
;
006,0,*Next known measuring block is 80.
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
03,0,Service Mode
;
07,0,Test Call
;
