;
; VAG-COM label file
;
; VW Passat (3B)
;
; component: J285 - instrument cluster (#17)
;
; p/n: 3B0-920-??2-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3B-17.LBL
; 3B0-920-xx2.LBL
;
; based on 3B0-920-822.LBL by Alberto Salvador (alberto.salvador@wanadoo.es - berto @ VW group related forums)
; updated/enhanced by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 03/25/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
;
001,0,Speed / Engine speed / Oil pressure / Time
001,1,Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2 (< min)
001,4,Time
;
002,0,Distance / Fuel / Ambient temperature
002,1,Mileage
002,2,Fuel Level (l)
002,3,Fuel Level Sender,Resistance
002,3,Ambient,Temperature (G17),only available with climatronic and/or multifunction display
;
003,0,Coolant and Oil
003,1,Coolant,Temperature
003,2,Oil Level,,Display Range: Ok/n.Ok
003,3,Oil,Temperature
;
050,0,Main Information
050,1,Mileage
050,2,Engine Speed
050,3,Oil,Temperature
050,4,Coolant,Temperature
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
125,4,Airbag
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,J285 - Instrument cluster
C1,??xxx - Additional equipment
C2,+00 - Without additional equipment
C3,+01 - Brake pad warning
C4,+02 - Seatbelt warning
C5,+04 - Washer fluid level warning
C6,+16 - Radio/Navigation
C7, 
C8,xx?xx - Country version
C9,1 - Europe / 2 - USA / 3 - Canada/Mexico/Latin America
C10,4 - England / 5 - Japan / 6 - Saudi Arabia / 7 - Australia
C11, 
C12,xxx?x - Service intervals
C13,0 - Fixed service intervals (PR-QG0)
C14,1 - Flexible service intervals (PR-QG1)
C15,2 - Fixed service interval (PR-QG2)
C16,3 - No service intervals
C17, 
C18,xxxx? - Distance impulse number (K-value)
C19,3 - 4134 - 6-Cylinder (Light armored vehicle)
C20,5 - 4182 - all other engines / 6 - 4128 - 8-Cylinder (W8)
;
