;
; VAG-COM label file
;
; VW Golf Convertible (1E) / VW Transporter (7D)
;
; component: central locking (#35)
;
; p/n: 7D0 959 800 A/B/C
;
; includes measuring blocks, coding and adaption
;
; by Sebastian Stange
; sebastian@ross-tech.com
;
; last modified: 12/15/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
; 
001,0,Basic Informations
001,1,System Voltage,(Terminal 30)
001,2,Ignition,(Terminal 15),Range: Term. 15 ON/Term. 15 OFF
001,3,Rotary Latch,Switch,Range: dr.closed/dr.open
001,4,Central Locking,Thermal Protection,Range: Yes/No
;
002,0,Vehicle Status
002,1,Remote Control,Key Buttons,Range: open/closed
002,2,Output,(closed),Range: open/n.operated
002,3,Output,(open),Range: open/n.operated
002,4,Vehicle,Status,Range: locked/unlocked
;
003,0,Remote Control Status
003,1,Permanent Code,Known,Range: OK/n.OK/n.meas.value
003,2,Variable Code,Known,Range: OK/n.OK/n.meas.value
003,3,Algorithm,,Range: OK/n.OK/n.meas.value
003,4,Key Number,,Range: 1...4
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Central Locking
C1,00001 - Standard
C2,00002 - Unknown
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A1,0,Remote Control Matching
A1,1,Key
A1,3,Count
A1,5,Remote Control Matching
A1,6,Enter the desired key count (maximum 4) as new value. Save.
A1,7,Then press and hold (for at least one second) the UNLOCK button on the fob
A1,8,at which time it will be learned. If you're programming more than one fob
A1,9,press and hold the UNLOCK button on the second fob for one second
A1,10,press and hold the UNLOCK button on the third fob for one second etc.
A1,11,You have a total of 15 seconds to do them all.
A1,12, 
A1,13,Note: To match additional keys increase the current key count.
A1,14, 
A1,15,Note: To overwrite existing keys first clear all existing keys. Channel 00 > Save
;
A02,0,Unlock Blink
A02,1,Unlock
A02,2,Blink
A02,3,Status
A02,5,Unlock Blink
A02,6,Blink when unlocking via remote control.
A02,7, 
A02,8,0 = off
A02,9,1 = on
;
A03,0,Lock Blink
A03,1,Lock
A03,2,Blink
A03,3,Status
A03,5,Lock Blink
A03,6,Blink when locking via remote control.
A03,7, 
A03,8,0 = off
A03,9,1 = on
;
