h;
; VAG-COM label file - 3D0-920-xxx-17.LBL
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
;
; Instrument Cluster - J285 - (#17)
;
;      p/n: 3D0 920 881  Component: KOMBIINSTRUMENT RB4 0312
;
; includes coding, adaptation & measured value blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3D-17.LBL
; 3D0-920-xxx-17.LBL
;
; by Sebastian Stange (sebastian@ross-tech.com) 12/06/2004
; modified 27/March/2005 by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; ready for VAG-COM 500.9 and above (500.9 supports block labels beginning with asterisks)
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,Common Information
001,1,Vehicle Speed,from brake module
001,2,Engine Speed,from transmission
001,3,Oil Pressure,,Specified Value: Oilpr.2 i.O.
001,4,Time of Day,(clock),Information taken from vehicle clock.
;
002,0,Common Information (continued)
002,1,Mileage,rounded
002,2,Fuel Tank,Total Contents
002,3,[N/A],,(see block 005 for fuel gauge information)
002,4,Outside Air,Temperature,Display Range: -45...+65 °C | +70 °C = short circuit | -50 °C = open circuit
;
003,0,Coolant and Oil Information
003,1,Coolant Temperature,from engine module
003,2,Oil Level
003,3,Oil Temperature,degrees C
;
004,0,Electrical Information
004,1,Battery Voltage
;
005,0,Fuel Sensors
005,1,Fuel Gauge,(G)
005,2,Fuel Level,Sensor 2 (G169)
005,3,Fuel Supply,Sensor 3 (G237)
005,4,Fuel Supply,Sensor 4 (G393)
;
006,0,Tank Content (Chambers)
006,1,Tank Content,(Main Chamber)
006,2,Tank Content,(Left Side)
006,3,Tank Content,(Right Side)
006,4,Tank Content,(Reserve)
;
007,0,Unknown
;Remark: Could this be oil level, or windshield fluid level? What about trip odometer?
;
008,0,Unknown
;
009,0,Unknown

010,0,*Next measuring block used is Group 50
;
050,0,Common Information
050,1,Mileage
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
051,0,*Next measuring block used is Group 60
;
060,0,Installation Information (Senders and Sensors)
;
061,0,Checking Installation Information
;
062,0,*Next measuring block used is Group 80
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
082,0,Flash-Tool-Code (FTC)
; Flash-Date (in dd.mm.yy)
;
083,0,*Next measuring block used is Group 125
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Airbag
;
127,0,CAN-Databus Communication (Powertrain)
127,3,Distance Control
;
128,0,CAN-Databus Communication (Powertrain)
128,1,Battery Monitoring
128,2,Electrical Ignition
128,3,Level Control
;
129,0,CAN-Databus Communication (Powertrain)
129,3,Brake Booster
;
130,0,CAN-Databus Communication (Comfort)
130,1,Comfort-CAN,Condition
130,2,Comfort system
130,3,Driver Door
130,4,Passenger Door
;
131,0,CAN-Databus Communication (Comfort)
131,1,Rear/Left Door
131,2,Rear/Right Door
131,3,Driver,Memory Seat
131,4,Electrical System
;
132,0,CAN-Databus Communication (Comfort)
132,2,Steering Wheel
132,3,Climate
132,4,Tire Pressure
;
133,0,CAN-Databus Communication (Comfort)
133,1,Roof Electronics
133,2,Passenger,Memory Seat
133,3,Rear,Memory Seat
133,4,Parking Aid
;
134,0,CAN-Databus Communication (Comfort)
134,2,Electrical Ignition
134,3,Wiper Electronics
;
135,0,CAN-Databus Communication (Comfort)
135,2,Display/Operation,Unit (front)
135,3,Display/Operation,Unit (rear)
;
136,0,Unknown
;
137,0,*Next measuring block used is Group 140
;
140,0,CAN-Databus Communication (Infotainment)
140,1,Infotainment-CAN,Condition
140,3,Radio/Navigation
140,4,Telephone
;
141,0,CAN-Databus Communication (Infotainment)
141,3,TV-Tuner
;
142,0,CAN-Databus Communication (Infotainment)
142,1,Display/Operation,Unit (front)
141,4,Telematics,(OnStar)
;
143,0,CAN-Databus Communication (Infotainment)
143,1,Digital,Sound Package
143,3,Parking Heater
143,4,Roof Electronics
;
136,0,*Next measuring block used is Group 201
;
201,1,K-Value
201,2,Wheel,Circumference
201,3,Starting impulse,recognized
;
202,1,Engine Hood,Switch
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton Instrument Cluster (Y24) Coding  
C01,??xxx - The SUM of all the codes for the warnings you want goes in the ?? field.
C02,+01 - Break Pad Wear Indicator active
C03,+02 - Fasten Seat Belt Warning active
C04,+04 - Low Windshield Washer Fluid Warning active
C05,+16 - Radio-Navigation installed (never applicable to North American Phaetons)
C06,+24 - Navigation display in Y24 (really should not be there - but it works)
C08,xx?xx - This number (choose one only) sets behavior by Country of operation.
C07,  
C09,1 - Europe, no 'key in ignition' door chime, default is kilometres
C10,2 - USA, 'key in ignition' door chime active, default is miles
C11,3 - Canada, 'key in ignition' door chime active, default is kilometres
C12,4 - Great Britain, no 'key in ignition' door chime, default is miles
C13,5 - Japan  6 - Saudi Arabia  7 - Australia
C14,NOTE: Default units of measure can be changed later by the driver via the SETTINGS button on J523.
C15, 
C16,xxx?x: This number (choose one only) determines how 'service now' warnings are generated.
C17,1 - Service Interval Display with flexible intervals (QG1 - normal for rest of world)
C18,2 - Service Interval Display with fixed intervals (QG2 - normal for North America) 
C19, 
C20,xxxx? - Distance Impulse Number (normally 1 - No further information available)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
A01,0,*Next adaptation channel available is 04
;
A02,0,Resetting Service Interval Reminder - change the value "1" to "0", test, then save.
;
A04,0,Instrument Cluster (Y24) Language selection
A04,1,
A04,5,Choose one language only
A04,6,1 - German
A04,7,2 - English
A04,8,3 - French
A04,9,4 - Italian
A04,10,5 - Spanish
A04,11,6 - Portuguese
A04,12,7 - Without text (symbols only)
A04,13,8 - Czech
A04,14, 
A04,15,NOTE 1: Not all languages listed above may be available.
A04,16,NOTE 2: This does NOT the affect infotainment screen (J523) language. The J523
A04,17,language choices depend on what is available from the navigation CD installed.
;
A05,0,*Next adaptation channel available is 09
;
A09,0,Mileage
A09,6,Mileage shown in the instrument cluster may be adapted upwards ONCE only.
A09,7,This is only done when a replacement (new) instrument cluster is installed
A09,8,in a Phaeton that has already been driven. A security access code may be needed.
;
A10,0,*Next adaptation channel available is 30
;
A30,0,Fuel Gauge Calibration
A30,5,Fuel Tank sensor
A30,6,Fuel Gauge calibration can be adjusted in increments of 1.
A30,7,The available range is from 108 to 148.
;
A31,0,*Next adaptation channel available is 35
;
;
; **************************************************
;
; Information related to Service Interval Reminders
;
; **************************************************
A40,0,Distance elapsed from last inspection in 100s of km
A40,5,Distance from inspection
A40,6,Resolution: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-48 must be
A40,9,entered and stored in the following order:
A40,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A41,0,Time elapsed from last inspection in days
A41,5,Time from inspection
A41,6, 
A41,7,NOTE: Adaptation channels 40-48 must be
A41,8,entered and stored in the following order:
A41,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A42,0,Minimum value mileage for next oil change
A42,5,Minimum value mileage
A42,6,Resolution: 1 unit = 1000 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-48 must be
A42,9,entered and stored in the following order:
A42,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A43,0,Maximum value mileage for next oil change
A43,5,Maximum value mileage
A43,6,Resolution: 1 unit = 1000 km
A43,7, 
A43,8,NOTE: Value should be 15 without longlife oil or 30 with longlife oil.
A43,9,
A43,10,NOTE: Adaptation channels 40-48 must be
A43,11,entered and stored in the following order:
A43,12,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A44,0,Maximum time interval for next oil change
A44,5,Maximum time interval in days
A44,6, 
A44,7,NOTE: Value should be 360 days without longlife oil or 720 days with longlife oil.
A44,8,  
A44,9,NOTE: Adaptation channels 40-48 must be
A44,10,entered and stored in the following order:
A44,11,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A45,0,Oil type (specification) - Indicate either Longlife or not Longlife
A45,5,Oil type
A45,6,Range available: 0.5 - 2.0
A45,7,NOTE: Value normally is:  1 = not longlife oil. 2 = longlife oil.
A45,8,
A45,9,NOTE: Adaptation channels 40-48 must be
A45,10,entered and stored in the following order:
A45,11,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A46,0,Total consumption amount (Gas only)
A46,0,Total consumption amount (Gas only)
A46,6, 
A46,7,NOTE: Adaptation channels 40-48 must be
A46,8,entered and stored in the following order:
A46,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A47,0,Soot entry (Diesel only)
A47,5,Soot entry (Diesel only)
A47,6,Resolution: 1 = 100 km
A47,7, 
A47,8,NOTE: Adaptation channels 40-48 must be
A47,9,entered and stored in the following order:
A47,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A48,0,Thermal load (Diesel only)
A48,5,Thermal load (Diesel only)
A48,6,Resolution: 1 = 100 km
A48,7, 
A48,8,NOTE: Adaptation channels 40-48 must be
A48,9,entered and stored in the following order:
A48,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A60,0,Undocumented (DATA-BUS Engine)
;35951
;
A61,0,Undocumented (DATA-BUS Comfort)
;447
;
A62,0,Undocumented (DATA-BUS Infotainment)
;28752
;
