;
; VAG-COM label file
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
; VW Bentley Continental GT - up to and including model year 2005 (not tested with this vehicle)
;
; component: Central Electronics -J519-  (#09)
;
; p/n: 3D0 937 049 E
;      3D0 937 049 G STG.Bordnetz 5001 Coding: 0000003 (same PN and component number on both Phaeton and Bentley)
;      3D0 937 049 H
;      NOTE: The Touareg is very different, therefore this file is not suitable for the Touareg.
;            Perhaps 50% of the MVB's are the same, but coding is totally different for the Touareg.
;            Use the existing file 7L6-937-049.lbl for the Touareg.
;
; includes measured value blocks, coding, and some (incomplete) information about adaptation.
;
; by Sebastian Stange (sebastian@ross-tech.com)
; modified by Michael Moore (moore99@rogers.com)
;
; last modified: 11/05/2004 (Sebastian)
; last modified: 27/March/2005 (Michael)
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,Light SWITCH status (not the status of the lights themselves)
001,1,Parking light,switch,Specified value: off/on
001,2,Low beam,light switch,Specified value: off/on
001,3,Automatic,headlight activation,Specified value: off/on
001,4,Switch for,emergency flasher,Specified value: active/inactive ('active' will only appear when switch is held in depressed position)
;
002,0,Light SWITCH status (not the status of the lights themselves)
002,1,Rear fog light,or VALET button,Specified value: off = not pressed at the moment/on = pressed in/not installed
002,2,Front Fog light,,off = not pressed at the moment/on = pressed in/not installed
002,3,Back-up light,switch,Specified value: off/on
002,4,[N/A]
;
003,0,Instrument panel illumination dimming
003,1,Increase,button,Specified value: active/inactive
003,2,Decrease,button,Specified value: active/inactive
003,3,Unknown
;
004,3,Engine hood,switch,Specified value: closed/open
;
005,0,Mirror adjustment switch
005,1,Y-Axis,(minus),Specified value: active/inactive
005,2,Y-Axis,(plus),Specified value: active/inactive
005,3,X-Axis,(minus),Specified value: active/inactive
005,4,X-Axis,(plus),Specified value: active/inactive
;
006,0,Mirror control switch position
006,1,Left mirror,selection,Specified value: active/inactive
006,2,Right mirror,selection,Specified value: active/inactive
006,3,Folding in,mirror,Specified value: active/inactive
006,4,Mirror Heating,switch,Specified value: active/inactive
;
007,0,Voltages present on the car
007,1,Terminal 15,(Ignition),Specified value: Term. 15 on/Term. 15 off
007,2,Terminal X,(consumers),Specified value: Term. X on/Term. X off
007,3,Power Supply,battery,Specified value: 6...15 V
007,4,Starter,battery,Specified value: 6...15 V
;
008,0,Status of the actual lamps themselves (not the switches for these lamps)
008,1,Left low,beam headlight,Specified value: off/on
008,2,Right low,beam headlight,Specified value: off/on
008,3,Left high beam,,Specified value: off/on
008,4,Right high beam,,Specified value: off/on
;
009,0,Status of the actual lamps themselves (not the switches for these lamps)
009,1,Left,parking light,Specified value: off/on
009,2,Right,parking light,Specified value: off/on
;
010,0,Status of the actual lamps themselves (not the switches for these lamps)
010,1,Turn signal,lights left,Specified value: off/on
010,2,Turn signal,lights right,Specified value: off/on
010,3,Front Fog lights,left/right,Specified value: off/on
;
011,0,Status of the switch position for turn signals or single side parking lights
011,1,Left turn,signal lever,Specified value: off/on
011,2,Right turn,signal lever,Specified value: off/on
011,3,Left parking,light switch,Specified value: off/on
011,4,Right parking,light switch,Specified value: off/on
;
012,0,Status of switch positions
012,1,Headlamp flash,to pass switch,Specified value: off/on
012,2,High beam switch,,Specified value: off/on
012,3,Switch for horn,,Specified value: off/on
012,4,Window washing,switch,Specified value: off/on
;
013,0,Load Management Intervention status
013,1,Load management,intervention,Specified value: active/inactive
013,2,max. reached,shut-off priority,Specified value: 0...254
;
014,0,Heated mirrors status
014,1,Driver door,heated mirror,Specified value: off/on
014,2,Passenger door,heated mirror,Specified value: off/on
;
015,0,Rotary traps (detents in the door latches that indicate the door is closed properly)
015,1,Driver door,rotary trap,Specified value: open/closed
015,2,Passenger door,rotary trap,Specified value: open/closed
015,3,Rotary trap,Left Rear door,Specified value: open/closed
015,4,Rotary trap,Right Rear door,Specified value: open/closed
;
016,0,Footwell light dimming levels, other vehicle conditions
016,1,Footwell light,dimming level,Specified value: 0...100 %
016,2,Terminal DFM,,Specified value: 0...255 %
016,3,Outside air,temperature,Specified value: 0...255 °
016,4,Gear Selector,lever position,Specified value: 0...15
;
017,0,Unknown value
017,2,Unknown
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton Central Electronics (J519) Coding
C01, 
C02,xxxx? - Choice of Daytime Running Light (DRL) Function
C03,Choose one number only from the list below
C04, 
C05,1 - Scandinavia - all lights illuminated for DRL + rear fog light installed.
C06,2 - North America - headlights only illuminated for DRL + no rear fog light installed.
C07,3 - No DRL of any kind (DRL feature disabled) + rear fog light installed.
C08, 
C09,NOTE 1: Interior light functions controlled by 'soft-buttons' such as dome lights illuminating 
C10,when doors are opened may need to be re-set after the DRL function has been changed. 
C11,Re-cycle the push-button(s) on the roof to the setting desired after recoding is done.
C12, 
C13,NOTE 2: Changing DRL selection away from 'North America' will cause loss of the valet
C14,lockout button function - this button will now be assigned to operate the rear fog light.
C15, 
;
;
;
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;Adaptation possibilities exist on channel 01, but the values and functions are not known. 
;On the author's 2004 North American W12, this value is 14.
;Could the values in this channel be the key to enabling the rear foglight, etc. as they are on the Touareg?
;No adaptation channels available 02 to 80 inclusive, did not check past 80.