;
; VAG-COM label file
;
; VW Passat (3B)
;
; component: J285 - instrument cluster (#17)
;
; p/n: 3B?-920-??9-???
;
; includes adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3B-17.LBL
; 3Bx-920-xx7.LBL
; 3Bx-920-xx9.LBL
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 04/April/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A2,0,Service reminder
A2,5,Service reminder reset
A2,6,displayed values:
A2,7,0 - no service
A2,8,1 - service
A2,9, 
A2,10,reset:
A2,11,0 - Service reminder reset
;
A4,0,Language for error messages and navigation (MFD only)
A4,5,Language for error messages and navigation
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,8 - Czech
;
A9,0,Dinstance (in 10km)
A9,1,Distance
A9,2,in 10
A9,3,km
A9,5,Distance changing
A9,6,Before the cluster accepts the new
A9,7,distance you have to login using 13861.
A9,8, 
A9,9,The distance can only be changed until
A9,10,the current value is not over 100km.
;
A21,0,Key count (Immobilizer)
;
A30,0,Fuel gauge adaption
A30,1,Current,value
A30,5,Fuel gauge adaption
A30,6,Basic value: 100
A30,7,Range: 120 - 136
A30,8,Unit: 1 Ohm
;
A35,0,Engine speed threshold
A35,5,Engine speed threshold adaption
A35,6,Basic value: 0
A35,7,Range: 0 - 1000
A35,8,Unit: 250 U/min
;
A40,0,Distance from inspection
A40,5,Distance from inspection
A40,6,Resolution: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-44 must be
A40,9,entered and stored in the following order:
A40,10,42 > 43 > 44 > 40 > 41
;
A41,0,Time from inspection
A41,5,Time from inspection
A41,6, 
A41,7,NOTE: Adaptation channels 40-44 must be
A41,8,entered and stored in the following order:
A41,9,42 > 43 > 44 > 40 > 41
;
A42,0,Minimum value mileage
A42,5,Minimum value mileage
A42,6,Resolution: 1 = 1000 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-44 must be
A42,9,entered and stored in the following order:
A42,10,42 > 43 > 44 > 40 > 41
;
A43,0,Maximum value mileage
A43,5,Maximum value mileage
A43,6,Resolution: 1 = 1000 km
A43,7, 
A43,8,NOTE: Adaptation channels 40-44 must be
A43,9,entered and stored in the following order:
A43,10,42 > 43 > 44 > 40 > 41
;
A44,0,Maximum time interval
A44,5,Maximum time interval
A44,6, 
A44,7,NOTE: Adaptation channels 40-44 must be
A44,8,entered and stored in the following order:
A44,9,42 > 43 > 44 > 40 > 41
;
A45,0,Oil quality
A45,5,Oil quality
A45,6,1 - Time or distance based service
A45,7,2 - Longlife service - Gasoline Engines
A45,8,4 - Longlife service - 4/6-Zyl.-TDI-Engines
A45,9, 
A45,10,NOTE: Adaptation channels 40-48 must be
A45,11,entered and stored in the following order:
A45,12,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A46,0,Total consumption amount (Gas only)
A46,0,Total consumption amount (Gas only)
A46,6, 
A46,7,NOTE: Adaptation channels 40-48 must be
A46,8,entered and stored in the following order:
A46,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A47,0,Soot entry (Diesel only)
A47,5,Soot entry (Diesel only)
A47,6,Resolution: 1 = 100 km
A47,7, 
A47,8,NOTE: Adaptation channels 40-48 must be
A47,9,entered and stored in the following order:
A47,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A48,0,Thermal load (Diesel only)
A48,5,Thermal load (Diesel only)
A48,6,Resolution: 1 = 100 km
A48,7, 
A48,8,NOTE: Adaptation channels 40-48 must be
A48,9,entered and stored in the following order:
A48,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
