;
; VAG-COM Measuring Block Labels file.
; S8 Central Locking
; Filename: 8L0-862-257-G.lbl
; 
; from 2001 Audi S8
;   Controller: 8L0 862 257 G  
;    Component: ZV-Pumpe, DWA, Funk D16
;       Module: 35
;       Coding: 15179
;
; **Modification History**
; Created:  Dave Eaton, 4th February 2004
; Modified: Dave Eaton, 5th February: Test & Corrections
; Corrections to: Dave.Eaton@clear.net.nz
;
; **********************************************************************
;
1,0,Overall Conditions #1 - See File
; Bit Positions
; X000 000 0000 0000 Unlock Driver/Passenger: 1=Key Activated 0=Key, in Centre Position
; 0X00 000 0000 0000 Lock Driver/Passenger: 1=Key Activated 0=Key, in Centre Position
; 00X0 000 0000 0000 Unlock Boot: 1=Key Activated 0=Key, in Centre Position
; 000X 000 0000 0000 Lock Boot: 1=Key Activated 0=Key, in Centre Position
; 
; 0000 X00 0000 0000 Rear Doors: 1=Open, 2=Closed
; 0000 0X0 0000 0000 Driver & Passenger Doors: 1=Open, 2=Closed
; 0000 00X 0000 0000 Bonnet: 1=Open, 2=Closed
;
; 0000 000 XX00 0000 Switch for Front Passenger Door Actuator: 00 = Not Actuated, 01 = Lock, 10=Unlocked, 11=N/A
; 0000 000 00XX 0000 Switch for Front Drivers Door Actuator: 00 = Not Actuated, 01 = Lock, 10=Unlocked, 11=N/A
;
; 0000 000 0000 X000 Boot Lid: 1=Open 2=Closed
; 0000 000 0000 0X00 Boot Light: 1=On 2=Off
; 0000 000 0000 00X0 Boot Unlocking Switch: 1=Actuated, 0=Not Actuated
; 0000 000 0000 000X Boot Lid Unlocking Motor: 1=Engine Running, 0=Engine Not Running
;
2,0,Further Conditions #2 - See File
; Bit Positions
; X000 0000 000 Interior Light Control: 1=Light On, 0=Light Off
; 0X00 0000 000 Sunroof Control: 1=Voltage Supplied, 0=Ground
; 00X0 0000 000 Comfort Close Function: 1=Activated 0=Not Activated
; 000X 0000 000 Comfort Open Function: 1=Activated 0=Not Activated
;
; 0000 X000 000 "Open" Radio Remote Control Switch: 1=Actuated, 0=Not Actuated
; 0000 0X00 000 "Close" Radio Remote Control Switch: 1=Actuated, 0=Not Actuated
; 0000 00X0 000 "Unlock Boot" Radio Remote Control Switch: 1=Actuated, 0=Not Actuated
; 0000 000X 000 "Panic" Radio Remote Control Switch: 1=Actuated, 0=Not Actuated
;
; 0000 0000 X00 Terminal 15: 1=Ignition on, 0=Ignition off
; 0000 0000 0X0 S Contact 1: 1=Contact on, 0=Contact Off
; 0000 0000 00X Ground Signal from Radio: 1=Radio INstalled, 0=Radio Removed
;
3,0,Further Conditions #3 - See File
; Bit Positions
; X 0000 0 0000 N/A
;
; 0 X000 0 0000 RC Key #4: 1=Address Occupied, 0=Not Occupied
; 0 0X00 0 0000 RC Key #3: 1=Address Occupied, 0=Not Occupied
; 0 00X0 0 0000 RC Key #2: 1=Address Occupied, 0=Not Occupied
; 0 000X 0 0000 RC Key #1: 1=Address Occupied, 0=Not Occupied
;
; 0 0000 X 0000 N/A
;
; 0 0000 0 X000 RC Button Open/Unlock: 1=Actuated, 0=Not Actuated
; 0 0000 0 0X00 RC Button Close/Lock: 1=Actuated, 0=Not Actuated
; 0 0000 0 00X0 RC Button Unlock Boot: 1=Actuated, 0=Not Actuated
; 0 0000 0 000X RC Button Panic: 1=Actuated, 0=Not Actuated
;
4,0,Further Conditions #4 - See File
; Bit Positions
; X00 0000 0000 0000 RC Activated: 1=Yes 0=No
; 0X0 0000 0000 0000 Operation of Safety CL with RC Remote: 1=No, 0=Yes
; 00X 0000 0000 0000 Comfort Fuction via RC Remote: 1=Yes, 0=No
;
; 000 X000 0000 0000 USA Door Logic: 1=Yes, 0=No
; 000 0X00 0000 0000 Hazard Light Confirmation of RC: 1=Yes, 0=No
; 000 00X0 0000 0000 Horn Confirmation of Anti-theft: 1=Yes, 0=No
; 000 000X 0000 0000 Hazard Light Confirmation of Close/Lock: 1=Yes, 0=No
;
; 000 0000 X000 0000 Tailgate Logic: 1=Yes, 0=No
; 000 0000 0X00 0000 Interior Monitoring OBD Capable: 1=No, 0=Yes
; 000 0000 00X0 0000 Locking of Vehicle via Vehicle Speed: 1=Yes, 0=No
; 000 0000 000X 0000 Vehicle is a Convertible: 1=Yes, 0=No
;
; 000 0000 0000 X000 Anti-theft Alarm Activated: 1=Yes, 0=No
; 000 0000 0000 0X00 Security CL Activated: 1=Yes, 0=No
; 000 0000 0000 00X0 Confirmation of ATWS via Hazards: 1=Yes, 0=No
; 000 0000 0000 000X N/A
;
;End of File