;
;  06A-906-019-XX
;
; Created by Kim Andersen:gasarm@post.tele.dk
; Engine code: AEH-AKL Golf 1998>,Bora 1999>
; ECU Number : 06A-906-019 
; Engine type: 1.6 I R4/2V SIMOS HS 2272
; Coding:04000
; Documentation used:"Erwin WorkShop Manual Golf 1998>,Bora 1999>
;                     Simos injection and ignition system"


0,0,Measured value blocks(Engine running at idle speed)click for details			
0,1,Intake air temperature		  , 84-158  = 15-71°Celius
0,2,Engine control unit supply voltage, 98-147  = 10-15 Volt
0,3,Coolant temperature 		  , 170-211 = 80-110°Celius
0,4,Air mass drawn in			  , 14-30   = 76-164 mg/lift
0,5,Lambda probe voltage		  , 0-50    = 0.0-1.0 Volt
0,6,Lambda learnt value at idling	  , 0-100   = -0.8-0.8 ms
0,7,Operation condition of Lanbda control-See measured value block 99
0,8,Throttle valve angle		  , 4-12    = 1.9-5.7°
0,9,Injection period			  , 2-4     = 2-4.1 ms.
0,10,Engine speed (idling speed)	  , 23-27   = 760-880 RPM
;
1,0,Basic functions-Click for  details 
1,1,Engine speed,,760-880 rpm 
1,2,Coolant,Temperature,80-110°Celius
1,3,Lambda,voltage,0.00-1.00 Volt
1,4,TBA valve,00000010,see lable file for details
;xxxxxxxx
;1        Fault identified by self-diagnosis
; 1       Signal from automatic gearbox
;  1      Air conditioner switched on
;   1     Idling speed switch open
;    1    Fault in Lambda control
;     1   Throttle valve open (angle check)
;      1  Engine running
;       1 Coolant temperature less than 80 °Celius
;
2,0,Basic Functions-Click for  details 
2,1,Engine speed,,760-880 rpm
2,2,Airflow,(engine load),76-164 mg/H
2,3,Road speed,
2,4,Engine,operating mode,see label file
;
;xxxx
;1    Overrun
; 1   Idling
;  1  Part throttle
;   1 Full throttle
;
3,0,Basic functions-Click for  details 
3,1,Engine speed,,760-880 rpm
3,2,Airflow, (engine load),76-164 mg/H
3,3,Throttle valve, angle, 1.9°-5.7°
3,4,Throt.valve, posi.duty cycle, -100-100 %
;
4,0,Basic functions-Click for  details
4,1,Engine speed,, 760-880 rpm 
4,2,Airflow,(engine load), 76-164 mg/H
4,3,Injection,period, 2.0-4.10 ms
4,4,Air mass, drawn in, 1.8 - 3.2 g/s

5,0,Basic functions-Click for  details
5,1,Engine Speed,,760-880 rpm
5,2,ECU,Voltage Supply, 10-15 Volt
5,3,Coolant,Temperature, 80-110°Celius
5,4,Intake air,Temperature, 15-71°Celius
;
6,0,Altitude adaption-Click for  details
6,1,Engine speed,, 760-880 rpm
6,2,Airflow,(engine load), 76-164 mg/H
6,3,Throttle valve, angle, 1.9°-5.7°
6,4,Altitude,correction factor,0.9-1.1
;
7,0,Idling adjustment-Click for  details
7,1,Throttle valve, angle,1.9°-5.7°
7,2,Idling learnt, value,0.95-1.05
7,3,Idling learnt, value,0.95-1.05
7,4,Engine,operating mode,see label file
;
;xxxx
;1    Overrun
; 1   Idling
;  1  Part throttle
;   1 Full throttle
;
8,0,Idling stabilitation-Click for  details
8,1,Engine speed,Actual,760-880 rpm  
8,2,Engine speed,specified,800-840 rpm
8,3,Idling control,,10-15 %
8,4,Amount of,air drawn in,1.0-3.2 g/s
;
9,0,Idling air requirements-Click for  details
9,1,Idling,control,10-15 %
9,2,Throttle valve, status,see label file
;xxxxxxxx
;0        Not allocated 
; 0       Not allocated
;  0      Not allocated
;   0     Not allocated
;    1    Fault has occurred during adaption
;     1   No current supply to throttle valve
;      1  Battery voltage too low (below 8V)
;       1 Idling switch open
;
9,3,Coolant,temperature,80-110°Celius
9,4,Engine speed,,760-880 rpm
;
10,0,Lambda control and activated charcoal filter system-Click for  details
10,1,Lambda, regulation,+25 to -25 % 
10,2,Lambda probe,Voltage,0.00-1.00 Volt
10,3,Activated charcoal, valve 1 Duty Cycle,0-20 %
10,4,Lambda correction, Tank venting active,-20-2 %
;
11,0,Lambda learning values-Click for  details
11,1,Injection,Period,2.00-4.10 ms
11,2,Lambda learnt, value idling,-0.1-1.0 ms
11,3,Lambda learnt, value part load,0.9-1.15 ms
11,4,Cond.tank, breather valve,see label file
;xxxxxxxx
;0        Vacant
; 1       Transition to vapour content check via fuel tank breather valve
;  1      Transition to fuel tank breather valve minimum operating level
;   1     Transition to fuel tank breather valve closure
;    1    Vapour content check via fuel tank breather valve
;     1   Fuel tank breather valve operating normally
;      1  Fuel tank breather valve minimum operating level
;       1 Fuel tank breather valve closed
;
12,0,Lambda control-Click for  details
12,1,Engine speed,760-880 rpm
12,2,Airflow,(engine load),76-164 mg/H
12,3,Lambda,regulation,-25% to +25 %
12,4,Lambda probe, Voltage,0.00-1.00 volt
;
13,0,Fuel consumption-Click for  details
13,1,Engine speed,,760-880 rpm
13,2,Airflow, (engine load),76-164 mg/H
13,3,Road speed,,0 km/h
13,4,Fuel consumption,,0.50-2.00 l/h
;
14,0,Knock control
14,1,Cyl 1,ign.angle retard,0.0°CA 
14,2,Cyl 2,ign.angle retard,0.0°CA 
14,3,Cyl 3,ign.angle retard,0.0°CA 
14,4,Cyl 4,ign.angle retard,0.0°CA 
;
15,0,Knock control
15,1,Engine speed,,760-880 rpm
15,2,Airflow,(engine load),76-164 mg/H
15,3,Cyl 1,ign.angle retard,0.0°CA 
15,4,Cyl 2,ign.angle retard,0.0°CA 
;
16,0,Knock control
16,1,Engine speed,,760-880 rpm
16,2,Airflow,(engine load),76-164 mg/H
16,3,Cyl 3,ign.angle retard,0.0°CA 
16,4,Cyl 4,ign.angle retard,0.0°CA 
;
17,0,Knock control - Knock Sensor Voltages 
17,1,Cyl 1,knock sensor,0.400-1.300 Vpt
17,2,Cyl 2,knock sensor,0.400-1.300 Vpt
17,3,Cyl 3,knock sensor,0.400-1.300 Vpt
17,4,Cyl 4,knock sensor,0.400-1.300 Vpt
;
18,0,Torque reduction for automatic gearbox
18,1,Engine speed,,760-880 rpm
18,2,Airflow,(engine load),74-164 mg/H
18,3,Ign.timing retard,gearbox cut-in,0.0°CA
18,4,Ignition timing,,6-14°BTDC
;
19,0,Operation condition
19,1,Engine speed,,760-880 rpm
19,2,Selector lever, pos.(0 or 1),0
19,3,Air conditioner,(0 or 1),0 
19,4,Operation condition,see label file
;xxxxxxxx
;0        Not allocated
; 0       Not allocated
;  0      Not allocated
;   0     Not allocated
;    0    Not allocated
;     1   Clutch pedal switch operated
;      1  Power steering pressure switch F88 activated
;       1 A/C compressor switched on
;
20,0,Lambda control operating condition
20,1,Engine speed,,760-880 rpm
20,2,Airflow,(engine load),76-164 mg/H
20,3,Coolant,Temperature,80-110°C
20,4,Operation condition,see label file
;xxxxxxxx
;1        Fault recorded in memory
; 0       Not allocated 
;  0      Not allocated
;   1     Restricted operation mode
;    1    Lambda control at limit
;     1   Lambda control switched on
;      1  Lambda probe functioning  
;       1 Mixture status: 1= Rich mixture 0= Lean mixture
;


21,0,Throttle valve control adaption - Click for  details
21,1,Throt.valve,control adaption,see label file;xxxxxxxx
;0        Not allocated			
; 0       Not allocated
;  0      Not allocated
;   0     Not allocated
;    1    Fault has occured during adaption
;     1   No current supply(duty cycle=0)
;      1  Battery voltage too low (below 8V)
;       1 Idling switch open
;
21,2,Throt.valve,min.position,70-100 %
21,3,Throt.valve,emerg.run.posi.,67-100 %
21,4,Throt.valve,max.position,0-20 %


22,0,Position of camshaft in relation to crankshaft
22,1,Engine speed,,760-880 rpm
22,2,Airflow,(engine load),76-164 mg/H
22,3,No.teeth,on Crk.sender,(- to +) 26-30
22,4,No.teeth,on Crk.sender,(+ to -) 86-90

57,0,Idling speed stabilisation-Air Compressor pressure signal-Click for  details
57,1,Engine speed,Actual,,760-880 rpm
57,2,Idling speed,Specified,Compressor: ON 800-920 /OFF 760-880 rpm 
57,3,A.C. Compres.,Mode,ON or OFF
57,4,G65, Duty Cycle,Compressor: ON 10-70% /OFF 1-5%

66,0,Cruise control system-Click for  details
66,1,Road speed,(actual),0 km/h
66,2,Brake clutch CCS, switch position,System 1000 For more see lable file
;xxxx
;1    Cruise control system available
; 1   Clutch pedal depressed/autom.gearbox always 1
;  1  Brake depressed or for autom.gearbox 
;     selector lever in "P" position and ignition switched on (engine stationary)
;   1 Brake depressed or for autom.gearbox
;     selector lever in "P" position and ignition switched on (engine stationary)
;
66,3,Road speed,(specified),0 km/h
66,4,Cruise Control,Swith Position,0000=0ff/0001=on  For more see lable file
;
;xxxx
;1    Resume speed,accelerate (CCS sliding switch at RES)
; 1   save speed/delay (SET button pressed)
;  1  CCS temporarily switched off{By brake or clutch),memory saved
;   1 CCS switched On
;
98,0,Matching throttle valve control part
98,1,Throttle Position,Sensor Voltage,3.70-4.75 Volt
98,2,Throttle Position,Actuator Voltage,2.28-4.75 Volt
98,3,Operating Mode,,00000000
98,4,Basic Setting,Status,00
;
99,0,Lambda regulation
99,1,Engine speed,,760-880 rpm
99,2,Coolant,temperature,80-110°C
99,3,Lambda, regulation,-25 to +25 %
99,4,Lambda,Operating condition,0xxx011x
;
;
;eor