;
; VAG-COM label file
;
; Audi A8 (4E)
;
; component: J104 - Brake Electronics (#03)
;
; p/n: 4E0 910 517 A/B
;
; includes measuring blocks
;
; by Sebastian Stange
; sebastian@ross-tech.com
;
; last modification: 09/23/2004
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,0,Wheel speed (largest value 20km/h (12.5 mph))
001,1,Front,Left
001,2,Front,Right
001,3,Rear,Left
001,4,Rear,Right
;
002,1,Brake test,switch
002,2,Brake light,switch
002,3,Parking,brake
002,4,ESP-button,(center console)
;
003,1,Engine speed,(RPM)
003,2,Engine torque,(Nm)
003,3,Engine torque,loss (Nm)
003,4,Throttle valve,angle (in %)
;
004,1,Standing time,,Display range: 0.0...255:59 h
004,2,EDL-shut-off
004,3,[N/A]
004,4,[N/A]
;
005,1,Steering,angle,Display range: -720...+720 ° (front wheels straight max. tolerance +/-5 °)
005,2,Rotation,rate,Display range: -69...+69 °/s
005,3,Brake,pressure,Display range: 0...292 bar
; -40 bar => short to Ground (GND)
; 290 bar => short to B+
005,4,Transverse,acceleration,Display range: -25...+25 m/sē
;
006,1,Voltage supply,terminal 15,Specified value: 9.8...17.4 V
006,2,Valve,relay
006,3,Activation,return flow pump
006,4,Workshop,code
;
007,0,Installation position - see labelfile (test applies only to room temperature)
; not OK => check brake temperature (test applies only to room temperature)
;        => Check installation of sensor (fully inserted, firmly screwed in)
;        => Check wheel bearing
;        => Check tolerance of axle
007,1,Front,Left,Display range: invalid/OK/not OK
007,2,Front,Right,Display range: invalid/OK/not OK
007,3,Rear,Left,Display range: invalid/OK/not OK
007,4,Rear,Right,Display range: invalid/OK/not OK
;
008,0,Direction of rotation
008,1,Front,Left,Display range: invalid/forward/reverse
008,2,Front,Right,Display range: invalid/forward/reverse
008,3,Rear,Left,Display range: invalid/forward/reverse
008,4,Rear,Right,Display range: invalid/forward/reverse
;
009,1,Brake test,switch 
009,2,Brake light,switch
009,3,Brake,pressure
009,4,[N/A]
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
125,0,CAN-Databus communication (Powertrain)
125,1,Steering,angle sensor
125,2,Transmission,Control Module
125,3,Engine,Control Module
125,4,Instrument,Cluster
;
126,0,CAN-Databus communication (Powertrain)
126,1,Adaptive Cruise,Control (ACC)
126,2,CAN-Gateway
126,3,Electric Parking,Brake (EPB)
126,4,Level Control,System
;
