;
; VAG-COM label file
;
; Audi A4 (8E)
;
; component: J234 - Airbag (#15)
;
; p/n: 8E0 959 655
;
; includes measuring blocks and (coding)
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 09/27/2004
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,1,Drivers-side,airbag,Display range: correct/too low/too high/endp. GND/endp. B+
001,2,Passenge-side,airbag,Display range: correct/too low/too high/endp. GND/endp. B+
001,3,belt tensioner,driver-side,Display range: correct/too low/too high/endp. GND/endp. B+
001,4,belt tensioner,passenger-side,Display range: correct/too low/too high/endp. GND/endp. B+
;
002,1,belt tensioner,driver-side rear,Display range: correct/too low/too high/endp. GND/endp. B+
002,2,belt tensioner,passenger-side rear,Display range: correct/too low/too high/endp. GND/endp. B+
002,3,belt tensioner,center rear,Display range: correct/too low/too high/endp. GND/endp. B+
002,4,[N/A]
;
003,1,voltage supply,Display range: correct/too low
003,2,[N/A]
003,3,seatbelt switch,driver-side,Display range: too low/too high/endp. GND/endp. B+/n.defined/belt YES/belt NO
003,4,seatbelt switch,passenger-side,Display range: too low/too high/endp. GND/endp. B+/n.defined/belt YES/belt NO
;
004,0,Belt usage recognition
004,1,driver-side,rear,Display range: too low/too high/endp. GND/endp. B+/n.defined/belt YES/belt NO
004,2,passenger-side,rear,Display range: too low/too high/endp. GND/endp. B+/n.defined/belt YES/belt NO
004,3,center,rear,Display range: too low/too high/endp. GND/endp. B+/n.defined/belt YES/belt NO
004,4,[N/A]
;
006,0,Igniter for side airbag
006,1,driver-side,front,Display range: correct/too low/too high/endp. GND/endp. B+
006,2,passenger-side,front,Display range: correct/too low/too high/endp. GND/endp. B+
006,3,driver-side,rear,Display range: correct/too low/too high/endp. GND/endp. B+
006,4,passenger-side,rear,Display range: correct/too low/too high/endp. GND/endp. B+
;
008,0,Igniter for head-level airbag
008,1,[N/A]
008,2,[N/A]
008,3,driver-side,,Display ange: correct/too low/too high/endp. GND/endp. B+
008,4,passenger-side,,Display range: correct/too low/too high/endp. GND/endp. B+
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
; Rest of world
; #############
;
; Series:  Front airbag, side airbag front, seat belt tensioner front, head airbag
;
; 0010602 - Series
; 0010702 - Series + rear side airbags
; 0011602 - Series + key switch to deactivate passenger airbag
; 0011702 - Series + rear side airbags + key switch to deactivate passenger airbag
;
; USA and Mexico
; ##############
;
; Series:  Front airbag, front side airbags, front seat belt tensioners, head airbag
;
; 0010605 - Series with 2 rear seat belt tensioners
; 0010705 - Series with 2 rear seat belt tensioners + rear side airbags
; 0010607 - Series with 3 rear seat belt tensioners
; 0010702 - Series with 3 rear seat belt tensioner + rear side airbags
;
