;
; VAG-COM label file 3D0-614-517.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 
;
; component: ABS Brake Electronics - J104 - (#03)
;
;       p/n: 3D0 614 517 R   Component: ESP 5.7 allrad H33 0043   Coding: 0008397 (W12 Phaeton - North America)
;
; includes measured value blocks
;
; by Sebastian Stange (Sebastian@ross-tech.com) - based on Sebastian's original work for file 8E0-614-517.lbl
; modified by Michael Moore (Moore@ross-tech.com) - tested for use on Phaeton, minor editorial corrections.
; with a tip of the hat to Dave Eaton (Dave.Eaton@clear.net.nz) for his pioneering work on the Audi S8 label file 4D0 907 389
;
; last modified: 09/26/2004 (Sebastian)
; last modified: 27/March/2005 (Michael) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; requires VAG-COM 500.9 or newer
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,Wheel speed (largest value 20km/h) - will read 1 km/h when parked.
001,1,Front Left
001,2,Front Right
001,3,Rear Left
001,4,Rear Right
;
002,0,Switch values affecting brake operation
002,1,Brake test,switch
002,2,Brake light,switch
002,3,Parking brake,status
002,4,ESP-button,status
;
003,0,General Engine Information
003,1,Engine speed,
003,2,Engine torque,
003,3,Engine torque,loss
003,4,Throttle valve,angle
;
004,1,Standing time,,Display range: 0.0...255:59 h
004,2,EDL-shut-off
004,3,[N/A]
004,4,[N/A]
;
005,0,General Vehicle Conditions
005,1,Steering,angle,Display range: -720...+720 ° (front wheels straight max. tolerance +/-5 °)
005,2,Rotation,rate,Display range: -69...+69 °/s
005,3,Brake,pressure,Display range: 0...292 bar
; -41 bar => short to Ground (GND)
; 290 bar => short to B+
005,4,Transverse,acceleration,Display range: -25...+25 m/sē
;
006,0,ABS Equipment Conditions
006,1,Voltage supply,terminal 15,Specified value: 9.8...17.4 V
006,2,Valve,relay;on - how it should be. off - not permitted.
006,3,Activation,return flow pump;off - how it should be. on - not permitted.
006,4,Workshop,code
;
007,0,Installation position - see labelfile (test applies only to room temperature)
; not OK => check brake temperature (test applies only to room temperature)
;        => Check installation of sensor (fully inserted, firmly screwed in)
;        => Check wheel bearing
;        => Check tolerance of axle
007,1,Front,Left,Display range: invalid/OK/not OK
007,2,Front,Right,Display range: invalid/OK/not OK
007,3,Rear,Left,Display range: invalid/OK/not OK
007,4,Rear,Right,Display range: invalid/OK/not OK
;
008,0,Direction of rotation
008,1,Front,Left,Display range: invalid/forward/reverse
008,2,Front,Right,Display range: invalid/forward/reverse
008,3,Rear,Left,Display range: invalid/forward/reverse
008,4,Rear,Right,Display range: invalid/forward/reverse
;
009,1,Brake test,switch,'Activated' shows when brake pedal is pressed
009,2,Brake light,switch,'Activated' shows when brake pedal is pressed
009,3,Brake Pressure
;
010,0*Next measuring block used is 080
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
125,0,CAN-Databus communication (Powertrain)
125,1,Steering,angle sensor
125,3,Transmission,Control Module
125,2,Engine,Control Module
125,4,Instrument,Cluster
;
