;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; component: Front Information Display Control Head (Big Infotainment Screen) - J523 - (#07)
;            sometimes also referred to as CCH (Central Control Head)
;
;       p/n: 3D0 035 008 M  Component: ZAB COCKPIT 0188 Coding: 0500305 (Phaeton - North America)
;
; includes coding & measured value blocks
;
; created by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; measuring block information added by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 30/March/2005
;
; ready for VAG-COM 402.3 and above
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
001,1,Battery Voltage,,Specification: 5.0...18.0 V
;
002,0,Signals
002,1,Status,Terminal 15
002,2,Status,S-Contact
002,4,Close-Request,S-Contact
;
003,1,Instrument,Illumination,Terminal 58d (Specification: 0...100 %)
003,2,Photo sensor,signal
;
004,0,HF Remote Supply
;
005,0,IF Remote Supply
;
006,1,Stereo channel 1,(left)
006,2,Stereo channel 1,(right)
;
007,1,Stereo cable 2,(Tel +)
007,2,Stereo cable 2,(Tel -)
;
008,1,Mono channel 3,(Nav +)
008,2,Mono channel 3,(Nav -)
;
009,1,Testing haptic,rotating adjuster
009,2,Testing left,rotating adjuster
009,3,Testing right,rotating adjuster
;
010,1,Testing keypad
;
011,1,Headphone,output 1 (left)
011,2,Headphone,output 1 (right)
;
012,1,Headphone,output 2 (left)
012,2,Headphone,output 2 (right)
;
013,1,Connection,CD-Changer
013,2,Malfunction,CD-Changer
;
014,2,Optical-Bus
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test numbers
;
082,0,FTC/Serial number
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton (3D) - Front Information Display Control Head - CCH - (J523) Coding
C01,xxxxxx?
C02,+1 Navigation Installed (J401 module)
C03,+2 Voice Activation Installed (for cell phone only - not for OnStar)
C04,+4 CD Changer Installed (R41 module)
C05, 
C06,xxxxx?x
C07,+1 TV Tuner Installed
C08,+2 Telephone Installed (cell phone - not OnStar)
C09,+4 Test Mode 1 selected
C10, 
C11,xxxx?xx
C12,+1 Seat Memory Installed
C13,+2 Tire Pressure Monitoring System installed
C14,+4 Parking Heater (Webasto overnight heater) installed
C15,
C16,x?xxxxx
C17,+0 None of the three configurations below
C18,+1 Rear Air Conditioning Control Head installed (typical)
C19,+2 Rear Central Control Head Installed (very rare)
C20,+4 Byte Coding Valid (always added to the total)
;
