; VAG-COM Measuring Block Labels file.
; Engine Codes ADY,AFT,AGG,AKR,AKS    
; 
; VW Golf, Vento, Passat, Cabrio, Corrado, Sharan
; Petrol Engine 2.0ltr, 4 cylinder - 8 valve
;
; ECU p/n  :  037 906 025 series  Simos Injection & Ignition System
;
; ADY,AGG,AKR  ECU known Suffix: -, A, D, F, G, H, P, Q, R, S, AC
;
; AFT,AKS      ECU known Suffix: T, AA
;
;
; Information sourced from VW Service Workshop Manual Edition 12.95
;
; Engines with Simos Injection 1992 onwards.
;
; *********************************
; ******Modification history*******
; *********************************
;
; Created:     Chris Gaskell, Stockport, UK.   22-June-2001
;              chrisgaskell@yahoo.com
;
; Note:        File set up for ADY,AFT,AGG engine codes
;              Engine codes AKR,AKS commented off
;              Swop commenting marks to switch on/off appropriate
;              measuring blocks
;
; File status: Untested, layout not proven
;              (but records of an 8v using basic VAG-COM agree)
;              (on 037 906 025D Corrado 8v 2.0ltr)
;
; Modified:    -
;
;
; *********************************
;
;0,0,Measuring block (Engine Codes ADY, AGG, AKR)
;0,1,Intake Air Temp,70...160 =4.5....72°C
;0,2,Batt Voltage,115...161 =12..16.5V
;0,3,Coolant Temp,120..150 =80...110 C
;0,4,Engine load,25...53 =9.75...19.5 %
;0,5,O2 Sensor,0...55 =0.00...1.10V
;0,6,O2 Sensor,0...22 =0...0.75ms
;0,7,Operating Cond.,not relevant
;0,8,Throttle Angle,5...14 =2.5...6.5<°
;0,9,Injection Time,2...4 =2...4ms
;0,10,Engine Speed,23...27 =736...864/min
;
;
;0,0,Measuring block (Engine Codes AFT, AKS)
;0,1,Intake Air Temp,70...160 =4.5....72°C
;0,2,Batt Voltage,115...161 =12..16.5V
;0,3,Coolant Temp,120..150 =80...110°C
;0,4,Engine load,30...45 =11.7...17.5 %
;0,5,O2 Sensor,10...50 =0.20...1.00V
;0,6,O2 Sensor,0...20 =0...0.64ms
;0,7,Operating Cond.,not relevant
;0,8,Throttle Angle,5...11 =2.5...4.7<°
;0,9,Injection Time,2...4 =2...4ms
;0,10,Engine Speed,24...28 =768...896/min
;
;
1,0,Engine Data (Adj. conditions) ADY, AGG, AKR
1,1,Engine Speed,750...850rpm
1,2,Coolant Temp,80...110°C
1,3,O2 Sensor,0.0 ... 1.1V
1,4,Adjust. Cond.,00000000
;                 1        -DTC recognised - in not yet memory,overrun
;                  1       -Signal Autobox, idling
;                   1      -Aircond on, part load
;                    1     -F60 Open,throttle valve idling switch
;                     1    -Fault in Lambda control
;                      1   -Throttle sw Open,.0-Throttle sw Close
;                       1  -Engine running
;                        1 -Coolant temp<80°C,0-Coolant temp>80°C
;
;
;1,0,Engine Data (Adj. conditions) AFT, AKS
;1,1,Engine Speed,780...880rpm
;1,2,Coolant Temp,80...110°C
;1,3,O2 Sensor,0.2 ... 1.0V
;1,4,Adjust. Cond.,00000000
;                 1        -DTC recognised - in not yet memory,overrun
;                  1       -Signal Autobox, idling
;                   1      -Aircond on, part load
;                    1     -F60 Open,throttle valve idling switch
;                     1    -Fault in Lambda control
;                      1   -Throttle sw Open,.0-Throttle sw Close
;                       1  -Engine running
;                        1 -Coolant temp<80°C,0-Coolant temp>80°C
;
;
2,0,General Engine Data  ADY, AGG, AKR
2;1,Engine Speed,750...850rpm
2,2,Injection Time,2...4ms
2,3,Battery Volts,12.0...16.5V
2,4,Intake Air Temp,15...55°C
;
;
;2,0,General Engine Data  AFT, AKS
;2;1,Engine Speed,780...880rpm
;2,2,Injection Time,2...4ms
;2,3,Battery Volts,12.0...16.5V
;2,4,Intake Air Temp,20...70°C
;
;
3,0,General Engine Data  ADY, AGG, AKR
3,1,Engine Speed,750...850rpm
3,2,Engine Load,9.75...19.5%
3,3,Throttle Angle,2.5...6.5 <°
3,4,Thottle Regl,6...21%
;
;
;3,0,General Engine Data   AFT,AKS
;3,1,Engine Speed,780...880rpm
;3,2,Engine Load, 12...17%
;3,3,Throttle Angle,3.0 ... 4.5 <°
;3,4,Thottle Regl,10...20%
;
4,0,Engine Data (Adj. conditions)ADY, AGG, AKR
4,1,Engine Speed,750...850rpm
4,2,Engine Load,9.75....19.5%
4,3,Vehicle Speed,0km/h
4,4,Operating Con.,00000000
;                  1        -DTC recognised - in not yet memory,overrun
;                   1       -Signal Autobox, idling
;                    1      -Aircond on, part load
;                     1     -F60 Open,throttle valve idling switch
;                      1    -Fault in Lambda control
;                       1   -Throttle sw Open,.0-Throttle sw Close
;                        1  -Engine running
;                         1 -Coolant temp<80°C,0-Coolant temp>80°C
;
;
;4,0,Engine Data (Adj. conditions)  AFT, AKS
;4,1,Engine Speed,780...880rpm
;4,2,Engine Load,12....17%
;4,3,Vehicle Speed,0km/h
;4,4,Operating Con.,00000000
;                  1        -DTC recognised - in not yet memory,overrun
;                   1       -Signal Autobox, idling
;                    1      -Aircond on, part load
;                     1     -F60 Open,throttle valve idling switch
;                      1    -Fault in Lambda control
;                       1   -Throttle sw Open,.0-Throttle sw Close
;                        1  -Engine running
;                         1 -Coolant temp<80°C,0-Coolant temp>80°C
;
;
5,0,Throttle Control (Lambda control) ADY, AGG, AKR
5,1,Engine Speed,750...850rpm
5,2,Charcoal Valve Duty,7...9%
5,3,Fuel Consumption,ms
5,4,Operating Cond.,Lambda 00000000  
;                          1         -Coding for synchro, mechanical emergency running
;                           1        -Not in use
;                            1       -Not in use
;                             1      -Lambda control at limit
;                              1     -Lambda control active
;                               1    -Fault in fault memory
;                                1   -Lambda probe operationally ready
;                                 1  -Rich mixture, 0=lean - idle switch open
;
;
;5,0,Throttle Control (Lambda control) AFT, AKS
;5,1,Engine Speed,780...880rpm
;5,2,Charcoal Valve Duty,7...9%
;5,3,Fuel Consumption,ms
;5,4,Operating Cond.,Lambda 00000000  
;                          1         -Coding for synchro, mechanical emergency running
;                           1        -Not in use
;                            1       -Not in use
;                             1      -Lambda control at limit
;                              1     -Lambda control active
;                               1    -Fault in fault memory
;                                1   -Lambda probe operationally ready
;                                 1  -Rich mixture, 0=lean - idle switch open
;
;
6,0,Lambda/Throttle Data   ADY, AGG, AKR
6,1,Learnt value 0-0.75ms,Lambda Cntrl-idle
6,2,Learnt value 0.90-1.1,Lambda Cntrl-part load
6,3,Learnt value 0.95-1.05,Throttle Valve-idle cntrl
6,4,Learnt value 0.95-1.05,Throttle Valve-Autobox
;
;
;6,0,Lambda/Throttle Data   AFT, AKS
;6,1,Learnt value 0-0.60ms,Lambda Cntrl-idle
;6,2,Learnt value 0.90-1.1,Lambda Cntrl-part load
;6,3,Learnt value 0.90-1.1,Throttle Valve-idle cntrl
;6,4,Learnt value 0.90-1.1,Throttle Valve-Autobox
;
;
7,0,Hall Sender Data    ADY, AGG, AKR
7,1,Hall - Engine Senders,57...60 or 1.0
7,2,Hall - Engine Senders,5...8
7,3,Altitude Correction,0.85 ... 1.15
7,4,Operating Cond.,Throttle 00000000
;                            1         -Coding for synchro, mechanical emergency running
;                             1        -Not in use
;                              1       -Not in use
;                               1      -Lambda control at limit
;                                1     -Lambda control active
;                                 1    -Fault in fault memory
;                                  1   -Lambda probe operationally ready
;                                   1  -Rich mixture, 0=lean - idle switch open
;
;
;7,0,Hall Sender Data    AFT, AKS
;7,1,Hall - Engine Senders,57...60 or 1.0
;7,2,Hall - Engine Senders,5...8
;7,3,Altitude Correctn,0.80 ... 1.20
;7,4,Operating Cond.,Throttle 00000000
;                            1         -Coding for synchro, mechanical emergency running
;                             1        -Not in use
;                              1       -Not in use
;                               1      -Lambda control at limit
;                                1     -Lambda control active
;                                 1    -Fault in fault memory
;                                  1   -Lambda probe operationally ready
;                                   1  -Rich mixture, 0=lean - idle switch open
;
;