;
; VAG-COM label file - 3D0-919-283.lbl
;
; Bentley Continental GT (3W) / VW Phaeton (3D)
;
; component: Park Distance Control -J446- (#76)
;
; p/n: 3D0 919 283 A
;      3D0 919 283 B
;      3D0 919 283 C Component: 03 Einparkhilfe 0807 Coding: 0000000 (Phaeton)
;      3W0 919 283   Component: 02 Einparkhilfe 0203 Coding: 0000000 (Bentley)
;      7L0 919 283 D Component: 33 Einparkhilfe 0806 Coding: 0000000 (Touareg) - via redirect file '7L-76.lbl'
;
;      fully tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; Includes measured value blocks and adaptation labels. No coding capabilities are know for this controller.
;
; This file is part of a redirection package,
; make sure you have both of the following files.
;
; 7L-76.LBL
; 3D0-919-283.lbl
;
; by Sebastian Stange (sebastian@ross-tech.com)
; modified by Michael Moore (Moore@ross-tech.com)
;
; last modified: 11/05/2004 (Sebastian)
; last modified: 27/March/2005 (Michael) 'PanEuropean' on the VW Vortex forum.
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,Direct echo from FRONT sensors - LEFT side
001,1,Sensor 1, front LEFT outside,Specified value: 20...60 cm (255 = invalid/unlimited)
001,2,Sensor 2, front LEFT center,Specified value: 20...120 cm (255 = invalid/unlimited)
001,3,Sensor 3, front LEFT inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
002,0,Direct echo from FRONT sensors - RIGHT side
002,1,Sensor 4, front RIGHT inside,Specified value: 20...150 cm (255 = invalid/unlimited)
002,2,Sensor 5, front RIGHT center,Specified value: 20...120 cm (255 = invalid/unlimited)
002,3,Sensor 6, front RIGHT outside,Specified value: 20...60 cm (255 = invalid/unlimited)
;
003,0,Cross echo from FRONT sensors
003,1,#1/2 left outside,to left center,Specified value: 20...70 cm (255 = invalid/unlimited)
003,2,#2/3 left center,to left inside,Specified value: 20...150 cm (255 = invalid/unlimited)
003,3,#3/4 left inside,to right inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
004,0,Cross echo from FRONT sensors continued
004,1,#4/5 right inside,to right center,Specified value: 20...150 cm (255 = invalid/unlimited)
004,2,#5/6 right center, to right outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
005,0,Distance value from FRONT sensors
005,1,#1/2 left outside,to left center,Specified value: 20...70 cm (255 = invalid/unlimited)
005,2,#2/3 left center,to left inside,Specified value: 20...150 cm (255 = invalid/unlimited)
005,3,#3/4 left inside,to right inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
006,0,Distance value from FRONT sensors continued
006,1,#4/5 right inside,to right center,Specified value: 20...150 cm (255 = invalid/unlimited)
006,2,#5/6 right center,to right outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
007,0,Direct echo from REAR sensors - RIGHT side
007,1,Sensor 7,rear RIGHT outside,Specified value: 20...60 cm (255 = invalid/unlimited)
007,2,Sensor 8,rear RIGHT center,Specified value: 20...120 cm (255 = invalid/unlimited)
007,3,Sensor 9,rear RIGHT inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
008,0,Direct echo from REAR sensors - LEFT side
008,1,Sensor 10,rear LEFT inside,Specified value: 20...150 cm (255 = invalid/unlimited)
008,2,Sensor 11,rear LEFT center,Specified value: 20...120 cm (255 = invalid/unlimited)
008,3,Sensor 12,rear LEFT outside,Specified value: 20...60 cm (255 = invalid/unlimited)
;
009,0,Cross echo from REAR sensors
009,1,#7/8 right outside,to right center,Specified value: 20...70 cm (255 = invalid/unlimited)
009,2,#8/9 right center,to right inside,Specified value: 20...150 cm (255 = invalid/unlimited)
009,3,#9/10 right inside,to left inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
010,0,Cross echo from REAR sensors continued
010,1,#10/11 left inside,to left center,Specified value: 20...150 cm (255 = invalid/unlimited)
010,2,#11/12 left center,to left outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
011,0,Distance value from REAR sensors
011,1,#7/8 right outside, to right center,Specified value: 20...70 cm (255 = invalid/unlimited)
011,2,#8/9 right center, to right inside,Specified value: 20...150 cm (255 = invalid/unlimited)
011,3,#9/10 right inside,to left inside,Specified value: 20...150 cm (255 = invalid/unlimited)
;
012,0,Distance value from REAR sensors continued
012,1,#10/11 left inside, to left center,Specified value: 20...150 cm (255 = invalid/unlimited)
012,2,#11/12 left center, to left outside,Specified value: 20...70 cm (255 = invalid/unlimited)
;
013,0,Total distances calculated for display and warning tone purposes
013,1,Left front corner,total distance,Specified value: 20...150 cm (255 = invalid)
013,2,Right front corner,total distance,Specified value: 20...150 cm (255 = invalid)
013,3,Right rear corner,total distance,Specified value: 20...150 cm (255 = invalid)
013,4,Left rear corner,total distance,Specified value: 20...150 cm (255 = invalid)
;
014,0,Voltages Present on PDC system
014,1,Supply voltage,,Specified value: 8.7...16.7 V
014,3,Sensor,supply voltage,Specified value: 7.2...9.2 V
014,4,Display-/speaker,supply voltage,Specified value: 7.5...16.5 V
;
015,0,Driver Control Inputs
015,1,PDC Off Button,status,Specified value: 0 = not pressed/1 = pressed
;
016,0,Vehicle Configuration Information
016,1,Automatic,transmission,Specified value: 0 = not installed/1 = installed
016,2,Gear selector,lever position,Specified values: 00/01/02/03/12/14
016,3,Parking,brake,Specified value: 0 = inactive/1 = active
;
017,0,Information about configuration of PDC system
017,1,Trailer,attached,Specified value: 0 = attached to car/1 = not attached to car
017,2,Trailer,control module,Specified value: 0 = not installed/1 = installed
017,3,Vehicle Speed,,Specified value: 0...250 km/h
017,4,Speed shut-off,,Specified value: 0 = inactive/1= active
;
018,0,Information about status of PDC system
018,1,Term 15 (Ignition),status,0 = off/1 = on
018,2,System status,,0 = inactive/1 = active
018,3,Display,brightness,Specified value: 50...100 %
018,4,Acoustic,warning,0 = inactive/1 = active
;
019,0,Unknown
;
;Remark: Could these be attenuation times?
;
020,0,Unknown
;
021,0,*End of known measuring blocks for this module.
;
;
;

;---------------------------------------------------
;
; Adaptation information
;
;---------------------------------------------------
;
;
A01,0,Front Warning Tone Volume
A01,5,Front Warning Tone Volume
A01,6,Adjustment of the front warning tone volume.
A01,7,
A01,8,Range: 0 - 100 %
;
A02,0,Rear Warning Tone Volume
A02,5,Rear Warning Tone Volume
A02,6,Adjustment of the rear warning tone volume.
A02,7, 
A02,8,Range: 0 - 100 %
;
A03,0,Shut-off speed
A03,5,Shut-off speed
A03,6,Adjustment of the vehicle speed for PDC shutdown.
A03,7, 
A03,8,Range: 1 - 15 kilometers per hour
A03,9,Standard value: 14
;
A04,0,Offset distance for rear bumper warnings
A04,5,Offset distance for rear bumper warnings
A04,6,Here you can enter an additional distance (in cm)
A04,7,to be added to rear measurements to allow for
A04,8,the presence of a trailer hitch or bicycle carrier.
A04,9, 
A04,10,Range: 1 - 30 cm
;
