;
; VAG-COM labelfile
;
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
; VW Caddy (2K) / VW Fox (5Z) / VW Golf/Jetta (1K) / VW Touran (1T)
;
; component: R - Radio (#56)
;
; p/n: 1K0 035 153 ?? - R 100
;      1K0 035 180 ?? - Premium 7
;      1K0 035 186 ?? - RCD 300
;      1K0 035 195 ?? - RCD 500
;      1Z0 035 161 ??
;      5M0 035 153 ?? - R 100
;      5M0 035 186 ?? - RCD 300
;      5M0 035 195 ?? - RCD 500
;      5P? 035 152 ??
;      5P? 035 186 ??
;      5Z0 035 152 ?? - R 200
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-56.LBL
; 5M-56.LBL
; 5P-56.LBL
; 5Z-56.LBL
; 1K0-035-1xx-56.LBL
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 03/26/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; Measuring block information
;
;---------------------------------------------------
;
;
001,1,Battery Voltage,(Terminal 30),Specification: 5...18 V
001,3,Dimming of,Radio Illumination,CAN-Message (Specification: ca. 29...98 %
001,4,S-Contact,Input Condition,CAN-Message
;
002,0,Telephone-Mute Analog-Input and CAN-Signal
;
003,0,Line-Out or Front Left Speaker
;
004,0,Line-Out or Front Right Speaker
;
005,0,Line-Out or Rear Left Speaker
;
006,0,Line-Out or Rear Right Speaker
;
007,0,Condition of Remote feed Antenna
;
008,0,Field Intensity of the currently adjusted Sender
;
010,0,Condition of 2nd Remote feed Antenna
;
011,0,Communication Status CD-Changer (R41)
;
015,0,Field Intensity of GSM Module
;
016,0,CAN Connection Satelite Radio Receiver (SDARS)
;
025,1,Internal,Malfunctions,see labelfile
; 01 = Button(s) jam
; 02 = Test sum error ROM / EPROM / Flash-ROM
; 03 = Test sum error EEPROM
; 04 = CC-Drive (Casette)
; 05 = CD-Drive
;
;
;---------------------------------------------------
;
; Adaptation information
;
;---------------------------------------------------
;
;
A01,0,Reception Optimization
A01,5,Reception Optimization
A01,6,This channel allows optimization of the reception
A01,7,behavior for areas with strong FM interference.
A01,8, 
A01,9,0 - Normal reception
A01,10,1 - Optimized reception
;
;
;---------------------------------------------------
;
; Coding information
;
;---------------------------------------------------
;
;
C0,Coding - Radio (R)
C1,?xxxx - Treble Speaker Monitoring
C2,1 - front and rear monitoring inactive
C3,2 - front monitoring active - rear monitoring inactive
C4,4 - front and rear monitoring active
C5,x?xxx - Telephone Control
C6,0 - no CAN-Telephone Control
C7,2 - CAN-Telephone Control
C8,xx?xx - Speaker channels
C9,0 - no passive speakers (sound system)
C10,2 - 2 passive speakers front and 0 passive speakers rear
C11,4 - 4 passive speakers
C12,xxx?x - Sound system correction
C13,0 - No sound system (no correction)
C14,1 - Sound system with cloth interior equipment
C15,2 - Sound system with leather interior equipment
C16,xxxx? - Radio configuration
C17,+2 - CD-Changer
C18,+4 - CAN-Secondary Display (Board Computer/large Display)
;
