;
; VAG-COM label file
;
; VW Caddy (2K) / VW Golf/Jetta (1K) / VW Touran (1T)
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
;
; component: J387 - Door Electronics (#52)
;
; p/n: 1K0 959 702 ???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1T-52.LBL
; 1K0-959-702.LBL
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 03/27/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,1,Window Regulator
001,1,WR-Button (E107),Passenger Door,Display Range: not operated/autom. open/autom. close/man. open/man. close
001,2,WR-Button (E81),Passenger Door,in Drivers Door (Display Range: not operated/autom. open/autom. close/man. open/man. close)
001,3,Window Regulator,Passenger Door,,Display Range: Up/Down/Position down/Position up/Excess temperature-shut-off/Pinch protection/End impact
001,4,Thermal Protection,Passenger Door,Display Range: Activated/inactive
;
002,1,Window Regulator,Comfort Control,Display Range: open/closed/not operated
002,2,Window Regulator,Enabling,Display Range: Yes/No
002,3,Dimming Value,(Terminal 58d),Display Range: 0...100 %
002,4,Vehicle Speed,,Specification: 0 km/h
;
003,1,Power Supply,(Terminal 30),Specification: 9.0...14.0 V
003,2,Databus,Condition,Specification: Dual Wire | Display Range: Single Wire/Dual Wire
003,3,Ignition,(Terminal 15),Display Range: Terminal 15 on/Terminal 15 off
003,4,S-Contact,,Display Range: operated/not operated
;
004,0,Dimming Values
004,1,Terminal 58s,,Display Range: 0...100 %
004,2,Interior Door,Handle Illumination,Display Range: 0...100 % /operated/not operated
004,3,Ambient,Illumination,Display Range: 0...100 %/operated/not operated
004,4,Internal,Illumination,Display Range: active/inactive
;
005,0,Central Locking - Passenger Door
005,1,Central Locking,Return Message,Display Range: locked/unlocked/safe
005,2,Rotary Switch,Passenger Door,Display Range: Door open/Door closed
005,3,Lock/Unlock Button,Passenger Door,Display Range: locking/unlocking/not operated/not installed
005,4,Key Switch,Passenger Door,Display Range: open/closed/not operated/not installed
;
006,0,Mirrors
006,1,Mirror Selector,Switch,Display Range: left/right/on (mirror heater switch)/off (mirror heater switch)/not operated
006,2,Mirror,Turn Signals,Display Range: active/inactive
006,3,Mirror,folded in,Display Range: active/inactive
006,4,Mirror Request,,Display Range: fold out/fold in/not operated
;
007,0,Mirrors
007,1,Mirror,Adjustment Switch,Display Range: Pos X+/Pos X-/Pos Y+/Pos Y-/not operated/not installed
007,2,Mirror Status,Position X,Display Range: 0...100 %
007,3,Mirror Status,Position Y,Display Range: 0...100 %
007,4,Mirror Supply,Potentiometer,Display Range: 0...100 % /active/inactive/not installed
;
008,1,Inside Door,Handle Button,Display Range: operated/not operated/not installed
008,2,Outside Door,Handle Button,Display Range: operated/not operated/not installed
008,3,Mirror Heater,,Display Range: 0...100 % /active/inactive (only active with engine running)
;
009,1,Opening Window,Regulator (locally),Display Range: 0...100 %
;
;
;---------------------------------------------------
;
; coding informations
;
;---------------------------------------------------
;
;
C0,J387 - Door Electronics (Passenger)
C1,+00002 - ambient mirror illumination
C2,+00004 - mirror turn signals
C3,+00008 - interior door handle illumination
C4,+00016 - manual-/automatic window run-down function
C5,+00032 - heated mirrors
C6,+00064 - door entry-/warning lamps
C7,+00256 - memory seats
C8,+00512 - right hand drive (RHD) vehicle
C9,+01024 - safe-motor
;
