;
; VAG-COM label file
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
; VW Bentley Continental GT - up to and including model year 2005 (not tested with this vehicle)
;
; Component: Steering Wheel Electronics -J453- (#16)
;
; p/n:    3D0 953 549 B
;         3D0 953 549 C
;         3D0 953 549 D
;         3D0 953 549 E - Component: Lenksäulenmodul 3401 (same PN and component number on both Phaeton and Bentley)
;         Not suitable for the Touareg - use existing file 7L6-953-549.lbl for Touaregs.  Phaeton and Touareg coding is the same, though.
;   
;
; includes measured value block and coding.
;
; by Sebastian Stange (sebastian@ross-tech.com)
; modified by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modified: 11/05/2004 (Sebastian)
; last modified: 27/March/2005 (Michael)
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,1,Turn signal,switch active,Specified value: not active/left/right
001,2,Headlamp flash,to pass active,Specified value: not active/active
001,3,High beam,switch active,Specified value: not active/active
001,4,Horn,switch depressed,Specified value: not active/active
;
002,1,Wiper Lever,Position,Specified value: not active/Interval/Level 1/Level 2
002,2,Wipe Interval,Dial,Specified value: off/Interval 1/2/3/Poti Ok
002,3,Front window,washing,Specified value: not active/active
002,4,Term 30 (Battery), Voltage
;
003,1,Steering column,adjustment,Specified value: not active/raise/lower/forward/backward
003,2,Easy Entry,switch,Specified value: on/off
;
004,0,CSO-Signal
004,1,Terminal P,,Specified value: on/off
004,2,Terminal S,,Specified value: on/off
004,3,Terminal X,(consumers),Specified value: on/off
004,4,Terminal 15,,Specified value: on/off
;
005,1,Term X (consumers),switched on,Specified value: yes/no
005,2,Steering wheel,heat status,Specified value: off/Level
005,3,St. wheel heater,via VSCM,Specified value: yes/no
005,4,St. wheel heater,via control head,Specified value: yes/no
;
006,0,Steering Wheel Heating
006,1,Steering wheel,heater status,Specified value: not installed/on/off
006,2,Temperature,sensor,Specified value: not installed/Temp. value
;
007,0,Steering Wheel Illumination
007,1,Dimming,value,steering wheel illumination
;
008,0,Unknown
;
;Remark: Check to see if 008 or 009 may have to do with steering wheel heating
;        or paddle shifter installation.
;
009,0,Unknown
;
010,0,Total Resistance Values for Switches Each Side of Steering Wheel Airbag
010,1,Left Side,buttons,value will vary depending on button that is pushed
010,2,Right Side,buttons,value will vary depending on button that is pushed
010,3,Unknown
;
011,0,Cruise Control System (CCS)
011,1,CCS+ switch,(resume),Specified value: not active/active
011,2,CCS- switch,(set),Specified value: not active/active
011,3,SET button,,Specified value: not active/active
011,4,RESUME,button,Specified value: not active/active
;
012,1,CANCEL,button,Specified value: not active/active
012,2,CCS ON/OFF,button,Specified value: not active/active
012,3,Illumination,button,Specified value: not pressed in/pressed in
012,4,Unknown
;
013,1,Vol+ button,,Specified value: not active/active
013,2,Vol- button,,Specified value: not active/active
013,3,Telephone,button,Specified value: not active/active
013,4,PTT button,,Specified value: not active/active
;
014,1,Right thumbwheel,depressed,Specified value: not active/active
014,2,Escape button,,Specified value: not active/active
014,3,Menu button,,Specified value: not active/active
;
015,1,Left thumbwheel,depressed
015,3,ADR (left),thumb wheel
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
125,0,CAN-Databus communication (Comfort)
125,1,Instrument,cluster
125,2,Central comfort,electric
125,3,Climate control
125,4,[N/A]
;
126,0,CAN-Databus communication (Comfort) - Door control modules
126,1,driver,side
126,2,passenger,side
126,3,rear,left,only with electrical power windows
126,4,rear,right,only with electrical power windows
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
; Remark:  Phaeton coding 232 (heated wheel), Bentley coding 212 (status unknown)   
;
C0,Steering wheel column electronics - J527 - 
;
C1,xx?xx - Additional equipment 
C2,0 - Steering wheel heating not installed
C3,1 - Steering wheel heating disabled  
C4,2 - Steering wheel heating enabled
C5,  
C6,xxx?x - Quantity of buttons on steering wheel
C7,0 - No buttons on steering wheel
C8,1 - 6 Cruise Control buttons, including GRA but not ADR
C9,2 - 6 Cruise Control buttons, including GRA and ADR thumbwheel
C10,3 - 4 Cruise Control buttons (normal for North America without ADR)
;
;REMARK: Security access activation code for retrofit installation of GRA (but not ADR) buttons is 11463
;
C11,  
C12,xxxx? - Electric Steering Column Adjustment
C13,1 - without electric steering column tilt and telescope
C14,2 - with electric steering column tilt and telescope
C15,
;
;
