***************************************************************************
********************** D720200 Design Resources Release *******************
***** All of the Software are under NDA or Software license agreement *****
***************************************************************************
 Release Note                                               December.1.2009
 
 NEC Electronics uPD720200
 USB 3.0 Host Controller Driver Kit (x86 and x64)
 for Windows XP, VISTA and 7
 
 Kit Version : 1.0.18.0 : December 1st, 2009
 Copyright (C) NEC Electronics Corporation 2009 All Rights Reserved
***************************************************************************

NOTE1:
 This installer package is generated with the InstallShield2010.
 If the previous driver package(v0.X.X.X , v1.0.1.0 or v1.0.7.0) is installed,
 please uninstall the previous driver package and install new package.


---------------------------------------------------------------------------
Table of Contents
---------------------------------------------------------------------------
1. Release Files
2. How to install
3. History

---------------------------------------------------------------------------
1. Release Files
---------------------------------------------------------------------------
Date        Time         Size   File Name                Version
--EXE(Installer Package)
 2009/12/01 15:03      7442KB   NECEL-USB3-Host-Driver-10180-setup.exe    1.0.18.0
 2009/09/11 16:06         1KB   setup.iss
 2009/12/01 11:01       954KB   InstallShield 2010 Projects-091201.zip

--ZIP
 2009/12/01 13:37      6930KB   NECEL-USB3-Host-Driver-10180-Setup-x86-x64-Binary.zip 1.0.18.0
---contents
 2009/09/11  9:10	 21KB	0x0C04.ini
 2009/09/11 14:50	 21KB	0x2C0a.ini
 2009/05/20 16:30        24KB   0x040a.ini
 2009/03/18 15:05	 22KB	0x040b.ini
 2009/05/20 17:27        25KB   0x040c.ini
 2009/03/16 14:23	 18KB	0x040d.ini
 2009/03/18 15:07	 22KB	0x040e.ini
 2009/05/20 16:46	 22KB	0x041b.ini
 2009/05/20 16:46	 22KB	0x041d.ini
 2009/03/18 15:15	 22KB	0x041e.ini
 2009/05/20 16:58	 22KB	0x041f.ini
 2009/05/20 16:55	 19KB	0x0401.ini
 2009/05/21 17:44        11KB   0x0404.ini
 2009/05/20 17:03	 22KB	0x0405.ini
 2009/05/20 17:03	 23KB	0x0406.ini
 2009/05/20 17:22        25KB   0x0407.ini
 2009/03/18 15:26	 26KB	0x0408.ini
 2009/05/21 15:53        21KB   0x0409.ini
 2009/05/20 17:06        24KB   0x0410.ini
 2009/06/08 16:45        15KB   0x0411.ini
 2009/03/16 14:28        14KB   0x0412.ini
 2009/05/20 17:07        24KB   0x0413.ini
 2009/05/20 17:08	 23KB	0x0414.ini
 2009/05/20 17:09	 23KB	0x0415.ini
 2009/05/20 17:09	 23KB	0x0416.ini
 2009/05/20 17:12	 22KB	0x0419.ini
 2009/05/20 17:13	 23KB	0x0424.ini
 2009/05/21 17:44        11KB   0x0804.ini
 2009/05/20 17:14        24KB   0x0816.ini
 2009/11/26 13:44	101KB	1025.mst
 2009/11/26 13:44        92KB   1028.mst
 2009/11/26 13:44       110KB   1029.mst
 2009/11/26 13:44       110KB   1030.mst
 2009/11/26 13:44       121KB   1031.mst
 2009/11/26 13:44       121KB   1032.mst
 2009/11/26 13:44        46KB   1033.mst
 2009/11/26 13:44       118KB   1034.mst
 2009/11/26 13:44       111KB   1035.mst
 2009/11/26 13:44       119KB   1036.mst
 2009/11/26 13:44	 69KB   1037.mst
 2009/11/26 13:44       115KB   1038.mst
 2009/11/26 13:44       119KB   1040.mst
 2009/11/26 13:44       114KB   1041.mst
 2009/11/26 13:44       107KB   1042.mst
 2009/11/26 13:44       115KB   1043.mst
 2009/11/26 13:44       108KB   1044.mst
 2009/11/26 13:44       114KB   1045.mst
 2009/11/26 13:44       113KB   1046.mst
 2009/11/26 13:44       110KB   1049.mst
 2009/11/26 13:44       111KB   1051.mst
 2009/11/26 13:44       107KB   1053.mst
 2009/11/26 13:44       106KB   1054.mst
 2009/11/26 13:44       109KB   1055.mst
 2009/11/26 13:44       112KB   1060.mst
 2009/11/26 13:44        91KB   2052.mst
 2009/11/26 13:44       114KB   2070.mst
 2009/11/26 13:44        47KB   3076.mst
 2009/11/26 13:44        47KB   11274.mst
 2009/11/26 13:44      4856KB   ISSetup.dll
 2009/12/01 15:05       781KB   nusb3drv.msi
 2009/12/01 15:05       968KB   setup.exe
 2009/11/26 13:44         3KB   Setup.ini
 2009/09/11 16:06	  1KB	setup.iss

 ----Files
 2009/11/20 19:17	 84KB	nusb3mon.dll             1.0.18.0
 2009/11/20 19:17	104KB	nusb3mon.exe             1.0.18.0
 2009/10/21 12:12       292KB   nusb3utl.exe		 1.0.15.0
 2009/10/26 23:22	 52KB   nusb3ver.dll		 1.0.18.0
 -----0C0A
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0C04
 2009/11/20 19:18         2KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----2C0A
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----040A
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----040B
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----040C
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----040D
 2009/11/20 19:19         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----040E
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----041B
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----041D
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----041E
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----041F
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0401
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0404
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0405
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0406
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----0407
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0408
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0409
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  3KB   nusb3utl.exe.mui
 -----0410
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0411
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0412
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0413
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0414
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----0415
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----0416
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0419
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----0424
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:12	  2KB   nusb3utl.exe.mui
 -----0804
 2009/11/20 19:18         3KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----0816
 2009/11/20 19:18         4KB   nusb3mon.exe.mui
 2009/10/21 12:13	  2KB   nusb3utl.exe.mui
 -----x64
 2009/11/26  3:47	  8KB	nusb3drv.cat
 2009/11/20 19:13	  3KB	nusb3drv.inf
 2009/11/20 19:15	 74KB	nusb3hub.sys             1.0.18.0
 2009/11/20 19:16	173KB	nusb3xhc.sys             1.0.18.0
 -----x86
 2009/11/26  3:47	  8KB	nusb3drv.cat
 2009/11/20 19:13	  3KB	nusb3drv.inf
 2009/11/20 19:15	 58KB	nusb3hub.sys             1.0.18.0
 2009/11/20 19:15	134KB	nusb3xhc.sys             1.0.18.0

---------------------------------------------------------------------------
2. Command Line Options
---------------------------------------------------------------------------
1)Silent install
 setup /s

 -To install this driver package silently, "setup.iss" file is needed.
  This package includes the "setup.iss" in which the following folder 
  path is set.
  "C:\Program Files\NEC Electronics\USB 3.0 Host Controller Driver".

  If you want to change install path, you need to generate setup.iss as
  follows: setup /r /f1".\setup.iss"

2)Checking existence of USB3.0 Host Controller

       /v"CHECK_HW_EXIST=1"

 -When this command line option is set, the installer checks existence of 
  the USB3.0 Host Controller(uPD720200). If the uPD720200 is not in the PC,
  this installer does not install the device drivers.
  ##Caution##
  To install the device drivers with this command line option after uninstalling
  the device drivers, it is necessary to restart on the PC.


---------------------------------------------------------------------------
3. History
---------------------------------------------------------------------------
---------------------------------------------------------------------------
 Version 1.0.18.0 : December 1st, 2009
---------------------------------------------------------------------------
We got Device Logo in the USB Controller Subcategory of the WLK1.4.

As for system logo test,
Microsoft announced testing process for USB3.0 xHCI Controller below.  
http://www.microsoft.com/whdc/whql/resources/news/whqlnews_112409.htm

- Windows Logo Information
  Submission ID: 1377656
  Product Name: NEC Electronics USB3 Host-01
  Category: Device
  Subcategory: Bus Controllers and Ports > USB Controller
  Qualification Level: Signature Only - Microsoft Windows XP family, x86 - Unclassified
                       Signature Only - Microsoft Windows XP family, x64 - Unclassified
                       Logo - Microsoft Windows Vista family, x86 Basic - Basic
                       Logo - Microsoft Windows Vista family, x64 Basic - Basic
                       Logo - Device - Compatible with Windows 7
                       Logo - Device - Compatible with Windows 7 x64

- The following bugs were fixed.
 1. When host driver is disabled and uPD720200 goes to D3hot state,
    CLKREQ# is not worked.

 2. When connectiong a certain Keyboard with fingerprint function, 
    PC can't enter S3/S4/S5 state.

 3. When using a certain ZIP Drive, file transfer is aborted.

---------------------------------------------------------------------------
 Version 1.0.17.0 : Nobember 2nd, 2009
---------------------------------------------------------------------------

- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1371310.

- The following bug was fixed.
   1. Function drivers were not unloaded when disconnectiong gold tree from
      the roothub port of USB3 HC. 

   2. After Warm Reset was issued, enumeration process might fail.

- InstallShield project file, License.rtf and versionDLL were updated.

- The following functions were added.
   1. When Link Errors frequently occur in the SuperSpeed-Port, driver changes 
      the connection from the SuperSpeed to HighSpeed.

   2. Transfer throughput was improved.

   3. Dynamic U1/U2 state control function was disabled. When enabling U1/U2 
      function, the device that SuperSpeed link with host is down was found.
      We decided to disable this function to get interoperability.
      To get certain interoperability, please use the FW version 3.0.2.1 
      released at Nov.2nd 2009 or later.

---------------------------------------------------------------------------
 Version 1.0.14.0 : October 6th, 2009
---------------------------------------------------------------------------

- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1358042.

- The following bug fixed.
   1. If the USB Device having multiple Endpoints with same EndpointAddress,
      the USB Device is not enumulated.

   2. The USB2.0 Device connected with mulitiple layered USB2.0 HUB is not detected
      after resuming Sleep and Hibernate.

- Updated InstallShield project file, script file, customDLL & versionDLL.

- Added the following functions to this installer.
   1. Command line option for checking existence of USB3.0 Host Controller.

       /v"CHECK_HW_EXIST=1"

     When this command line option is set, the installer checks existence of 
     the USB3.0 Host Controller(uPD720200). If the uPD720200 is not in the PC,
     this installer does not install the device drivers.

     ##Caution##
     To install the device drivers with this command line option after uninstalling
     the device drivers, it is necessary to restart on the PC.

   2. Previously, this installer does not install device drivers to the PC
      in which device drivers with same version is already installed.
      In this version, it reinstalls the device drivers to the PC.

---------------------------------------------------------------------------
 Version 1.0.12.0 : September 11th, 2009
---------------------------------------------------------------------------
- Updated End User Licence Agreement.

- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1349589.

- This package includes "Install Shield 2010 Project Files" in the EXE folder
  with which any cusotmers can customize install package.

- Installer Wizard Messages, "nusb3mon.exe" and "nusb3utl.exe" support 
  the following languages.

  LCID : Language
   0401 : Arabic
   0404 : Traditional Chinese
   0405 : Czech
   0406 : Danish
   0407 : German
   0408 : Greek
   0409 : English
   040A : Spanish (Traditional)
   040B : Finnish
   040C : French
   040D : Hebrew
   040E : Hungarian
   0410 : Italian
   0411 : Japanese
   0412 : Korean
   0413 : Dutch
   0414 : Norwegian (Bokmal)
   0415 : Polish
   0416 : Portuguese (Brazilian)
   0419 : Russian
   041B : Slovak
   041D : Swedish
   041E : Thai
   041F : Turkish
   0424 : Slovenian
   0804 : Simplified Chinese
   0816 : Portuguese(Standard)
   0C04 : Chinese (Hong Kong)
   0C0A : Spanish (Modern)
   2C0A : Spanish (Latin America)

- The following bug fixed.
   1. Bluescreen sometimes occurs when starting WebCam application.

   2. The mouse supported SelectiveSuspend function does not work when 
      it wakes up from suspend state.

   3. Can't access CD-ROM Media in a Blu-Ray Drive.

- Optimized SS/HS bulk transfer performance

---------------------------------------------------------------------------
 Version 1.0.10.0 : August 26th, 2009
---------------------------------------------------------------------------
- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1346130.

- All of files except for the CAT files are same as Version1.0.10.0 Beta2

---------------------------------------------------------------------------
 Version 1.0.10.0Beta2 : August 24th, 2009
---------------------------------------------------------------------------
- This version includes Microsoft TestSigned CAT Files.
  Note: If this driver package is used on x64 Windows Vista/7,
        need to set the following command. 
        >bcdedit -set TESTSIGNING ON

- This installer package is generated with the InstallShield2010.
  If the previous driver package(v0.X.X.X , v1.0.1.0 or v1.0.7.0) is installed,
  please uninstall the previous driver package and install new package.

- Installer Wizard Messages, "nusb3mon.exe" and "nusb3utl.exe" support 
  the following languages.

  LCID : Language
   404 : Traditional Chinese
   407 : German
   409 : English
   40A : Spanish
   40C : French
   410 : Italian
   411 : Japanese
   412 : Korean
   413 : Dutch
   804 : Simplified Chinese
   816 : Portuguese(Standard)

- The following bug fixed.
   1. Some hub devices does not detected after resuming Sleep and Hibernate.

   2. Bluescreen occurs after resuming Sleep and Hibernate.

- Known issue. This issue will fixed at next version.
   1. Bluescreen sometimes occurs when strting WebCam application.

---------------------------------------------------------------------------
 Version 1.0.7.0Beta : July 17th, 2009
---------------------------------------------------------------------------
- The following bug fixed.

1. USB Devices are not detected after resuming from Sleep and Hibernate.

2. Bluescreen occurs after resuming from Sleep and Hibernate.

3. USB-VGA Devices does not work correctly.

4. The message that bandwidth is getting low might not be indicated.

-The following function Added
1. Add a Vender Defined Command. 

---------------------------------------------------------------------------
 Version 1.0.1.0Beta : June 15th, 2009
---------------------------------------------------------------------------
- This package includes the following applications.
  1. nusb3mon.exe
  This application provides the following function 
  USB3.0 Specificatin Section 11.1 indicates the follwoing function.
  To address the situation where a USB 3.0 device is connected to a
  USB 2.0-only port on a USB 3.0- capable host, after establishing a
  USB 2.0 high-speed connection with the device, it is recommended
  that the host inform the user that the device will support
  SuperSpeed operation if it is moved to a USB 3.0-capable port on the
  same host. If a USB 3.0 device is connected to a USB 3.0- capable
  host via a USB 2.0 hub, it is recommended that the host inform the
  user that the device will support SuperSpeed operation if it is
  moved to an appropriate host port or if the hub is replaced with a
  USB 3.0 hub.

  2. nusb3ver.exe 
  This application provides functions that shows Driver Version 
  and Firmware Version.

- The following bug fixed.

1. Function driver is not unloaded after resuming from Sleep and Hibernate.

2. USB Remote wake up function is not worked correctly.

3. Bluescreen occured when repeating hot-pulg of FS-Speaker Device 
   that is connected with HS-Hub that is connected with USB3.0 HC.

---------------------------------------------------------------------------
 Version 0.9.12.0Beta : May 29th, 2009
---------------------------------------------------------------------------
- Changed installer package configuration.

  1. EXE type
     *All files are included in the EXE file.
     *Combined x86 and x64 in one package.

  2. ZIP type
     *Conposed of 3 contents, setup.exe, x86 folder and x64 folder.
     *All files for x86 are in x86 folder.
     *All files for x64 are in x64 folder.
     *Setup.exe installs drivers automatically.

---------------------------------------------------------------------------
 Version 0.9.12.0Beta : May 27th, 2009
---------------------------------------------------------------------------
- The following bug fixed.

1. Function driver is not unloaded after resuming from Sleep and Hibernate.

2. When repeating hot-pulg of a USB2.0 device, the device is not detected.

3. When connecting two USB Devices and after resuming from Sleep and Hibernate,
   both devices is not detected.

4. Bluescreen occuerd when USB-VGA device is running.

5. Dual Display mode of a USB-VGA device can't be operated.

---------------------------------------------------------------------------
 Version 0.9.4.0Beta : March 27th, 2009
---------------------------------------------------------------------------
- Support for Super Speed Transactions

---------------------------------------------------------------------------
 Version 0.9.3.0Beta : March 9th, 2009
---------------------------------------------------------------------------
- The following bug fixed.

1. If the system is booted up with a USB device already present on the USB 
   port, the USB port is in-operative and cannot be recovered even if the 
   USB device is unplugged and then plugged back in.

---------------------------------------------------------------------------
 Version 0.9.0.0Beta : February 9th, 2009
---------------------------------------------------------------------------
- First Beta Version Release

---------------------------------------------------------------------------
