; 4B0-907-357.LBL file
; version 2003 Aug. 17
;
; for (xenon) head lights range adjusting module (PR-8Q2)
; 4B0 907 357 module mainly used in Passat and A3/A4/A6/TT designed until year 2001
; (4BO 907 357 C module used short period for PR-8Q3 in other VAG cars)
;
; Made by Alberto Salvador (Spain/EU), alberto.salvador@wanadoo.es , berto @ VW group related forums
;
1,0,Voltages and Speed
1,1,Power Supply,Voltage
1,2,Main Beam Voltage,-56b- pin
1,3,Speed,( Km/h )
;
2,0,Axles sensors and Adaptation
2,1,Front level sensor,-G78- Voltage
2,2,Rear level sensor,-G76- Voltage
2,3,Adaptation [O.K.],(Run/ON=Leveling)
;
; If adaptation it's OK should display "ADP. O.K."
; "ADP. ON" or "ADP. Run" it's displayed while
; leveling motors (-V48- and -V49-) are adjusting headlights