;
; VAG-COM label file - 3D0-919-887.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
;
; component: Control Module for Navigation with CD Mechanism - J401 - (#37)
;
;       p/n: 3D0 919 887 A  Component: NAVIGATION 0147 Coding: 0400000 (Phaeton - North America)
;
;       Part Numbers for Other Platforms (it is not known whether this label file will work with these)
;          7L6 919 887 A Component: Navigation 0627 Coding: 0000002 (Touareg - North America)
;          7L6 919 887 A Component: Navigation 0634 Coding: 0000002 (Touareg - North America)
;          7L6 919 887 B Component: Navigation 0627 Coding: 0000002 (Touareg - North America)
;          7L6 919 887 D Component: Navigation 0628 Coding: 0000002 (Touareg - North America)
;          3W0 919 887 A Component: NAVIGATION 0168 Coding: 0400000 (Bentley Continental GT - North America)
;
;
; includes coding & measured value blocks
;
; by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modification: 20/March/2005
;
; ready for VAG-COM 402.3 and above
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Phaeton Control Module for Navigation with CD Mechanism - J401
C1,x?xxxxx
C2,4 - Byte Code Valid
C3,0 - No Byte Code
C4, 
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
;Data exists in blocks 001 to 006 inclusive, but it is not documented.
;VAG-COM 500.9 is very slow to read some of these blocks, be patient.
;
001,0,General Vehicle Information
001,1,Supply,voltage
;
002,0,Inputs used by Navigation System
002,1,Unknown
002,2,Unknown
002,3,Reverse signal,for dead reckoning,
;
003,0,GPS Antenna Status (On-glass Rear Window Antenna - not the OnStar shark-fin)
;
004,0,Satellite Related Information
004,2,Satellites,in view now,
004,3,Number of channels,for tracking
;
005,0,Wheel circumference for measuring distance when satellite signal is lost.
;
006,0,Unknown
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;Remark: Security access is required to adapt this controller.
;
;


