;
; VAG-COM Measuring Block Labels file.
; Module 76 -- Parking aid rear  4-channel
; A3 , A4 , A6 , A8
;
; p/n  :  4B0-919-283
;
; **Modification history**
; created:  Dima Suhov, 20 July 2002.
; please email any comments or corrections: terma@svitonline.com
;
; **********************************************************************
1,0,Distance sensor:
1,1,rear left,cm
1,2,rear left/centre,cm
1,3,rear right/centre,cm
1,4,rear right,cm
;
2,1,Shortest distance,cm
2,2,Road speed,km/h
2,3,Warning buzzer
2,4,---
;
3,1,Supply voltage,V
3,2,Reverse gear
3,3,Trailer
3,4,---
;
4,0,Attenuation time:
4,1,rear left,ms
4,2,rear left/centre,ms
4,3,rear right/centre,ms
4,4,rear right,ms
;
5,0,END
;
6,0,END
;
7,0,END
;
;
;<end of file>
