;
; VAG-COM label file
;
; Bentley Continental GT (3W) / VW Phaeton (3D)
;
; component: Battery Charger -J367-  (#71)
;
; p/n: 3D0 915 181 A
;      3D0 915 181 B Component: Batteriemanagement 2600 (Phaeton)
;      3D0 915 181 C Component: Batteriemanagement 2700 (Bentley)
;
; includes measured value blocks. This component does not support coding or adaptation.
;
; by Sebastian Stange (sebastian@ross-tech.com)
; modified by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modified: 11/05/2004 (Sebastian)
; last modified: 27/March/2005 (Michael)
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,Voltages Present
001,1,Term 15 (Ignition),(start relevant),Specified value: 0...16.5 V
001,2,Terminal 30,(start relevant),Specified value: 0...16.5 V
001,3,Terminal 30,(Supply battery),Specified value: 0...16.5 V
001,4,Terminal 30,(starter battery),Specified value: 0...16.5 V
;
002,0,Current Demands
002,1,Current,Term 15 (Ignition),start relevant
002,2,Current,Term 30 (Battery),start relevant
002,3,Battery compartment,temperature
002,4,Internal battery, temperature
;
003,0,Digital inputs
003,1,Digital input,Term 15 (Ignition),Specified value: Term. 15 on/Term. 15 off
003,2,Digital input,Term 50 (Starter),Specified value: Term. 15 on/ Term. 15 off
003,3,Digital input,Key In,Specified value: on/off
;
004,0,*This group not used.
;
005,0,Engine Related Information
005,1,Engine Speed
005,2,Temperature,of generator
005,3,Unknown
;
006,0,Unknown - could this be intervention load management status?
006,1,Unknown
006,2,Battery warning,indication lamp,Status = on or off
;
007,0,*Next measuring block used is block 80.
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0*End of documented measuring blocks for this module.
;Remark: No further blocks up to 105, did not check beyond that/
;
