;
; VAG-COM label file 3D0-907-135.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
;
; component: Roof Electronics -J528-  (#38)
;
; p/n: 3D0 907 135 B Component: Dachmodul 0605  Coding: 0000015
;
; includes measured value blocks, coding, and adaptation
;
; by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modified: 27/March/2005 (Michael)
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
;Remark: Data exists many blocks, but it is not fully documented
;
;
001,0,Power Supply to Controller
001,1,Voltage
;
002,0,Cabin Dome Lights
002,2,Front Cabin,% Illumination
002,4,Rear Cabin,% Illumination
;
003,0,Front Seat Reading Lights
003,3,Driver Seat,% Illumination
003,4,Passenger Seat,% Illumination
;
004,0,Rear Seat Reading Lights
004,3,Left Rear Seat,% Illumination
004,4,Right Rear Seat,% Illumination
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton Roof Electronics (J528) Coding
C01,xxxxx?? - Sum up all the applicable codes to get the correct number
C02,
C03,+00 - Standard (non solar reflecting) safety glass on cabin windows
C04,+01 - Automatic headlight control (tunnel symbol on light switch and speedometer)
C05,+02 - Inside rear view mirror with memory capability
C06,+04 - Cabin interior anti-theft monitoring
C07,+08 - Normal electric operated sunroof
C08,+16 - Solar power generating sunroof for unattended ventilation
C09,+24 - Solar radiation reflecting glass on cabin windows
C10,+32 - No sunroof at all (solid steel roof)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
;Remark: Channels 11, 12, 13 are used, but the function of these is unknown.
;
;Channel 11 value = 58474
;Channel 12 value = 8824
;Channel 13 value = 13520
;
;Above values taken from a 2004 W12 North American Phaeton.
;
;
;
