;
; VAG-COM label file
;
; VW Caddy (2K) / VW Golf/Jetta (1K) / VW Touran (1T)
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
;
; component: J453 - Steering Wheel Electronics (#16)
;
; p/n: 1K0 953 549 ???
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8P-16.LBL
; 1K0-953-549.LBL
;
; by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 03/23/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,1,Blinker,,Display Range: n. operated/left/right
001,2,Headlamp Flasher,,Display Range: n. operated/operated
001,3,High Beam,,Display Range: n. operated/operated
001,4,Front Wiper,,Display Range: n. operated/level/Stage Int./Stage 1/Stage 2
;
002,1,Interval Stages,,Display Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Display Range: n. operated/operated
002,3,Wiping Rear,,Display Range: n. operated/operated/not installed
002,4,Washing Rear,,Display Range: n. operated/operated/not installed
;
003,1,Terminal Status,,see labelfile
; ?xxxx - P-Contact
; x?xxx - S-Contact
; xx?xx - Terminal 75
; xxx?x - Terminal 15
; xxxx? - Terminal 50
003,2,Horn,,Display Range: n. operated/operated
003,3,Multi-Function,Display,Display Range: n. installed/n. operated/Reset/Up/Down
;
004,0,Cruise-Cntrol-System
004,1,Main Switch,,Display Range: n. installed/off/on
004,2,CCS-Set,,Display Range: n. operated/decelerate/accelerate/Reset
;
005,1,Park Position in,Selector Lever,Display Range: n. installed/n.Ok/on/recognized
005,2,Selector Lever,Information (Pos. P),Display Range: n. defined/recognized/on
005,3,Key,Removal Lock,Display Range: n. installed/on/off
005,4,Status Key,Removal Lock,Display Range: n. installed/Ok/n.Ok
;
006,0,Multi-Function Steering Wheel
006,1,Communication,,Display Range: n. intalled/Ok/n.Ok
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Display Range: yes/no
;
007,0,Multi-Function Steering Wheel
007,1,Buttons pressed
007,2,Buttons pressed
007,3,Tiptronic Down,,Display Range: n. operated/operated/not installed
007,4,Tiptronic Up,,Display Range: n. operated/operated/not installed
;
008,1,Steering Wheel,Heater,Display Range: n. installed/off/on
008,2,Temprature,Sensor,Display Range: n. installed/Temperature
008,3,Current,at Output
008,4,Driverside,heated Seat,Display Range: off/Stage
;
009,1,Dimming,,Display Range: 0...100 %
;
