;
; VAG-COM Measuring Block Labels file.
; S8 Immobiliser Movement Detector
; Filename: 4d0-951-177-b.lbl
; 
; from 2001 Audi S8
;   Controller: 4D0 951 177 B  
;       Module: 45
;    Component: Innenraumueberw.    D06
;       Coding: 00001
;
; **Modification History**
; Created:  Dave Eaton, 3rd February 2004
; Modified: Dave Eaton, 5th February: Test & Corrections
; Corrections to: Dave.Eaton@clear.net.nz
;
;
; **********************************************************************
22,0,Immobiliser: Status
22,1,Start permitted,(1 - Yes)
22,2,ECM Responding,(1 - Yes)
22,3,Key Condition,(1 - Yes)
22,4,Number of keys,Adapted (<=8)
;
23,0,Immobiliser: Keys
23,1,Variable code,Auth. (1 - Y)
23,2,Key Status,Trans. (1 - Locked)
23,3,Fixed code,Auth. (1 - Y)
23,4,Immobilizer Status,(6 -norm. see file)
; 4 - Customer Service New i.e. delivery condition
; 5 - Customer Service Locked
; 6- Anti-theft Immobiliser adapted, normal functioning condition
; 7- Key adaption active
;
24,0,Immobiliser: Lockout Times (minutes)
24,1,Instrument,Cluster
24,2,Engine Control,Module
24,3,Emergency,Release
24,4,Transponder,Recognition
;
;End of File